Circuit: * C:\keyterm\git\amplifier_6c\03_lm3886_amp\06_simulation\Active_balanced_reciever.asc

WARNING: Less than two connections to node AMP_OUT_SUPER.  This node is used by R17.
Direct Newton iteration failed to find .op point.  (Use ".option noopiter" to skip.)
Starting Gmin stepping
Gmin = 10
Gmin = 1.07374
vernier = 0.5
vernier = 0.25
vernier = 0.125
vernier = 0.0625
Gmin = 1.08884
vernier = 0.03125
vernier = 0.015625
Gmin = 1.03122
vernier = 0.0078125
vernier = 0.0104167
vernier = 0.00520833
Gmin = 1.01724
vernier = 0.00260417
vernier = 0.00347222
Gmin = 1.01042
vernier = 0.00173611
vernier = 0.00231481
vernier = 0.00115741
Gmin = 1.00852
vernier = 0.00154321
vernier = 0.000771604
Gmin = 1.00667
vernier = 0.00102881
vernier = 0.000514403
vernier = 0.00068587
Gmin = 1.00542
vernier = 0.000514403
vernier = 0.00068587
vernier = 0.000514402
Gmin = 1.00461
Gmin = 0
Gmin stepping failed

Starting source stepping with srcstepmethod=0
Source Step = 3.0303%
Source Step = 33.3333%
Source Step = 63.6364%
Source Step = 93.9394%
Source stepping succeeded in finding the operating point.

.step drive_voltage=0
Heightened Def Con from 0.00199975 to 0.00199975
Heightened Def Con from 0.00199975 to 0.00199975
Heightened Def Con from 0.00199975 to 0.00199975
Heightened Def Con from 0.00399975 to 0.00399975
.step drive_voltage=0.5
.step drive_voltage=1
.step drive_voltage=1.5
.step drive_voltage=2
