Circuit: * C:\keyterm\git\amplifier_6c\03_lm3886_amp\06_simulation\sound_impairment_monitor.asc

R27: both pins shorted together -- ignoring.
R3: both pins shorted together -- ignoring.
WARNING: Specified period is not longer than the sum of Trise, Tfall, and Ton for v§lin_in.  Increasing period to 0.00033
WARNING: Node NC_01 is floating.

WARNING: Less than two connections to node NC_01.  This node is used by C2.
WARNING: Less than two connections to node DRIVE.  This node is used by V2.
WARNING: Less than two connections to node LIN_REF.  This node is used by V§LIN_REF.
WARNING: Less than two connections to node LIN_IN.  This node is used by V§LIN_IN.
Direct Newton iteration failed to find .op point.  (Use ".option noopiter" to skip.)
Starting Gmin stepping
Gmin = 10
Gmin = 1.07374
vernier = 0.5
vernier = 0.25
vernier = 0.125
vernier = 0.0625
Gmin = 1.08884
vernier = 0.03125
vernier = 0.015625
Gmin = 1.03122
vernier = 0.0078125
vernier = 0.0104167
vernier = 0.00520833
Gmin = 1.01724
vernier = 0.00260417
vernier = 0.00347222
Gmin = 1.01042
vernier = 0.00173611
vernier = 0.00231481
vernier = 0.00115741
Gmin = 1.00852
vernier = 0.00154321
vernier = 0.000771604
Gmin = 1.00667
vernier = 0.00102881
vernier = 0.000514403
vernier = 0.00068587
Gmin = 1.00542
vernier = 0.000514403
vernier = 0.00068587
vernier = 0.000514402
Gmin = 1.00461
Gmin = 0
Gmin stepping failed

Starting source stepping with srcstepmethod=0
Source Step = 3.0303%
Source Step = 33.3333%
Source Step = 63.6364%
Source Step = 93.9394%
Source stepping succeeded in finding the operating point.


Date: Fri Oct 14 14:20:38 2022
Total elapsed time: 0.946 seconds.

tnom = 27
temp = 27
method = modified trap
totiter = 8492
traniter = 2643
tranpoints = 613
accept = 453
rejected = 160
matrix size = 159
fillins = 193
solver = Normal
Thread vector: 5.4/4.3[4] 3.6/2.9[4] 2.1/1.5[2] 0.6/0.9[1]  2592/500
Matrix Compiler1: 16.33 KB object code size  3.7/2.0/[0.8]
Matrix Compiler2: 16.06 KB object code size  1.8/2.5/[0.5]

