Circuit: * C:\Users\Edwin\Documents\19_git\Amplifier_6C\01_volume\06_simulation\DigitalVolumeControl.asc

C5: both pins shorted together -- ignoring.
WARNING: Less than two connections to node 3.3V.  This node is used by V3.
WARNING: Less than two connections to node ZEROCROSS.  This node is used by A1.
Direct Newton iteration failed to find .op point.  (Use ".option noopiter" to skip.)
Starting Gmin stepping
Gmin = 10
Gmin = 1.07374
Gmin = 0.115292
Gmin = 0.0123794
Gmin = 0.00132923
Gmin = 0.000142725
Gmin = 1.5325e-005
Gmin = 1.6455e-006
Gmin = 1.76685e-007
Gmin = 1.89714e-008
vernier = 0.5
vernier = 0.25
Gmin = 5.50669e-009
vernier = 0.125
vernier = 0.0625
Gmin = 5.09126e-009
vernier = 0.0833333
vernier = 0.111111
Gmin = 4.0318e-009
vernier = 0.148148
vernier = 0.197531
Gmin = 2.78655e-009
vernier = 0.263374
Gmin = 1.56737e-009
vernier = 0.351165
vernier = 0.46822
Gmin = 6.07574e-010
vernier = 0.624294
vernier = 0.832392
Gmin = 1.39744e-010
vernier = 1
Gmin = 1.71975e-011
Gmin = 1.84656e-012
Gmin = 1.98273e-013
Gmin = 0
Gmin stepping succeeded in finding the operating point.


Date: Sat May 28 22:01:05 2022
Total elapsed time: 10.603 seconds.

tnom = 27
temp = 27
method = modified trap
totiter = 105832
traniter = 104505
tranpoints = 26750
accept = 18596
rejected = 8154
matrix size = 195
fillins = 240
solver = Normal
Thread vector: 62.2/50.8[4] 25.2/19.6[2] 12.0/8.7[4] 1.4/2.7[1]  2592/500
Matrix Compiler1: 23.03 KB object code size  14.9/7.8/[4.9]
Matrix Compiler2: 23.78 KB object code size  8.1/10.9/[1.6]

