(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "SN74AUP2G08" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 5.715 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SN74AUP2G08" (id 1) (at -11.43 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:VSSOP-8_2.4x2.1mm_P0.5mm" (id 2) (at 0.635 27.305 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup2g08.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1651354031059&ref_url=https%253A%252F%252Fwww.ti.com%252Fgeneral%252Fdocs%252Fsuppproductinfo.tsp%253FdistId%253D10%2526gotoUrl%253Dhttps%253A%252F%252Fwww.ti.com%252Flit%252Fgpn%252Fsn74aup2g08" (id 3) (at -23.495 29.845 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "man" "Ti" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "man_no" "SN74AUP2G08DCUR" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "dist" "" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "dist_no" "" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "SN74AUP2G08_0_1"
      (rectangle (start -5.715 12.065) (end 5.08 -11.43)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start -1.905 -9.525) (mid 1.905 -5.715) (end -1.905 -1.905)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start -1.905 0.635) (mid 1.905 4.445) (end -1.905 8.255)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -6.35 -8.255)
          (xy -4.445 -8.255)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -6.35 1.905)
          (xy -4.445 1.905)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -4.445 -3.175)
          (xy -6.35 -3.175)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -4.445 6.985)
          (xy -6.35 6.985)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.905 -5.715)
          (xy 4.445 -5.715)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.445 4.445)
          (xy 1.905 4.445)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.905 -1.905)
          (xy -4.445 -1.905)
          (xy -4.445 -9.525)
          (xy -1.905 -9.525)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.905 8.255)
          (xy -4.445 8.255)
          (xy -4.445 0.635)
          (xy -1.905 0.635)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "SN74AUP2G08_1_1"
      (pin input line (at -8.89 6.985 0) (length 2.54)
        (name "1A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 1.905 0) (length 2.54)
        (name "1B" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 6.985 -5.715 180) (length 2.54)
        (name "2Y" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -0.635 -13.97 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 -3.175 0) (length 2.54)
        (name "2A" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 -8.255 0) (length 2.54)
        (name "2B" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 6.985 4.445 180) (length 2.54)
        (name "1Y" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -0.635 14.605 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
