(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "2130830005" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -12.7 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "2130830005" (id 1) (at -6.35 -1.27 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "818_USB:MOLEX_2130830005" (id 2) (at 35.56 22.86 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 -13.97 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "PARTREV" "A" (id 4) (at 43.18 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "STANDARD" "Manufacturer recommendations" (id 5) (at 35.56 20.32 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "Molex" (id 6) (at 44.45 31.75 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.36mm" (id 7) (at 46.99 26.67 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (symbol "2130830005_0_0"
      (rectangle (start -12.7 17.78) (end 12.7 -16.51)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin power_in line (at 2.54 -21.59 90) (length 5.08)
        (name "GND_A" (effects (font (size 1.016 1.016))))
        (number "A1" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 5.08 -21.59 90) (length 5.08)
        (name "GND_A" (effects (font (size 1.016 1.016))))
        (number "A12" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 22.86 270) (length 5.08)
        (name "VBUS_A" (effects (font (size 1.016 1.016))))
        (number "A4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 8.89 180) (length 5.08)
        (name "CC1" (effects (font (size 1.016 1.016))))
        (number "A5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 3.81 180) (length 5.08)
        (name "DA+" (effects (font (size 1.016 1.016))))
        (number "A6" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 1.27 180) (length 5.08)
        (name "DA-" (effects (font (size 1.016 1.016))))
        (number "A7" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -6.35 180) (length 5.08)
        (name "SBU1" (effects (font (size 1.016 1.016))))
        (number "A8" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 5.08 22.86 270) (length 5.08)
        (name "VBUS_A" (effects (font (size 1.016 1.016))))
        (number "A9" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 7.62 -21.59 90) (length 5.08)
        (name "GND_B" (effects (font (size 1.016 1.016))))
        (number "B1" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 10.16 -21.59 90) (length 5.08)
        (name "GND_B" (effects (font (size 1.016 1.016))))
        (number "B12" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 7.62 22.86 270) (length 5.08)
        (name "VBUS_B" (effects (font (size 1.016 1.016))))
        (number "B4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 6.35 180) (length 5.08)
        (name "CC2" (effects (font (size 1.016 1.016))))
        (number "B5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -3.81 180) (length 5.08)
        (name "DB+" (effects (font (size 1.016 1.016))))
        (number "B6" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -1.27 180) (length 5.08)
        (name "DB-" (effects (font (size 1.016 1.016))))
        (number "B7" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -8.89 180) (length 5.08)
        (name "SBU2" (effects (font (size 1.016 1.016))))
        (number "B8" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 10.16 22.86 270) (length 5.08)
        (name "VBUS_B" (effects (font (size 1.016 1.016))))
        (number "B9" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -10.16 -21.59 90) (length 5.08)
        (name "SHELL_GND" (effects (font (size 1.016 1.016))))
        (number "SH1" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -7.62 -21.59 90) (length 5.08)
        (name "SHELL_GND" (effects (font (size 1.016 1.016))))
        (number "SH2" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -5.08 -21.59 90) (length 5.08)
        (name "SHELL_GND" (effects (font (size 1.016 1.016))))
        (number "SH3" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -2.54 -21.59 90) (length 5.08)
        (name "SHELL_GND" (effects (font (size 1.016 1.016))))
        (number "SH4" (effects (font (size 1.016 1.016))))
      )
    )
  )
  (symbol "MOLEX 2130830005" (in_bom yes) (on_board yes)
    (property "Reference" "J?" (id 0) (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MOLEX 2130830005" (id 1) (at 0 29.21 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at -21.59 -10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at -21.59 -10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MOLEX 2130830005_0_1"
      (arc (start -11.43 15.24) (mid 8.0822 7.1578) (end 0 26.67)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start -0.635 20.32) (end 0.635 -21.59)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 0 -27.94) (mid 8.0822 -8.4278) (end -11.43 -16.51)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -11.43 -16.51)
          (xy -11.43 15.24)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 15.24)
          (xy 11.43 -16.51)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 0 26.67) (mid -8.0822 7.1578) (end 11.43 15.24)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 11.43 -16.51) (mid -8.0822 -8.4278) (end 0 -27.94)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "MOLEX 2130830005_1_1"
      (pin free line (at -13.97 12.7 0) (length 2.54)
        (name "A1_GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -10.16 0) (length 2.54)
        (name "A10_RX2-" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -12.7 0) (length 2.54)
        (name "A11_RX2+" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at -13.97 -15.24 0) (length 2.54)
        (name "A12_GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at 13.97 12.7 180) (length 2.54)
        (name "B1_GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 13.97 10.16 180) (length 2.54)
        (name "B2_TX2+" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 13.97 7.62 180) (length 2.54)
        (name "B3_TX2-" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 5.08 180) (length 2.54)
        (name "B4_VBUS" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 13.97 2.54 180) (length 2.54)
        (name "B5_CC2" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 0 180) (length 2.54)
        (name "B6_D+" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 -2.54 180) (length 2.54)
        (name "B7_D-" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -13.97 10.16 0) (length 2.54)
        (name "A2_TX1+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 13.97 -5.08 180) (length 2.54)
        (name "B8_SBU2" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.97 -7.62 180) (length 2.54)
        (name "B9_VBUS" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 -10.16 180) (length 2.54)
        (name "B10_RX1-" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 13.97 -12.7 180) (length 2.54)
        (name "B11_RX1+" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at 13.97 -15.24 180) (length 2.54)
        (name "B12_GND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at 13.97 -29.21 180) (length 2.54)
        (name "mount_1" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at 13.97 -31.75 180) (length 2.54)
        (name "mount_2" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at 13.97 -34.29 180) (length 2.54)
        (name "mount_3" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at 13.97 -36.83 180) (length 2.54)
        (name "mount_4" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -13.97 7.62 0) (length 2.54)
        (name "A3_TX1-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 5.08 0) (length 2.54)
        (name "A4_VBUS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -13.97 2.54 0) (length 2.54)
        (name "A5_CC1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -13.97 0 0) (length 2.54)
        (name "A6_D+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -13.97 -2.54 0) (length 2.54)
        (name "A7_D-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -13.97 -5.08 0) (length 2.54)
        (name "A8_SBU1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -7.62 0) (length 2.54)
        (name "A9_VBUS" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
