(footprint "Phoenix_TDPT2,5_POS_3_P5,08" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61F848A3)
  (attr through_hole)
  (fp_text reference "REF**" (at 6.35 -8.89 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 39a8cd39-294a-4c8a-99d7-71b35feea45f)
  )
  (fp_text value "PhoenixContact_TDPT_2,5_1x3_P5,08mm_Horizontal" (at 2.54 -15.24 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 74bc92af-f8ba-4546-8ffd-4a067527e0e8)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 16d2d7a7-7b51-4707-8d4b-74e0cabd17f9)
  )
  (fp_line (start -5.08 -7.62) (end -6.35 -8.89) (layer "F.SilkS") (width 0.12) (tstamp 0db0eefe-b1f9-488c-b4c4-78d287c16d0a))
  (fp_line (start -3.81 -8.89) (end -5.08 -7.62) (layer "F.SilkS") (width 0.12) (tstamp 2859b683-ea3f-4f02-9bf8-9591485ad1e4))
  (fp_line (start -8.02 11.34) (end 8.02 11.34) (layer "F.SilkS") (width 0.12) (tstamp 44b6a7c7-45d5-478d-af77-087040a31db1))
  (fp_line (start -8.02 -6.66) (end -8.02 11.34) (layer "F.SilkS") (width 0.12) (tstamp 478e1d5f-3361-4094-b60f-abe6a720cf4e))
  (fp_line (start -8.02 -6.66) (end 8.02 -6.66) (layer "F.SilkS") (width 0.12) (tstamp 766ddc19-af5a-4e09-a63d-aa90e0de5dee))
  (fp_line (start 8.02 11.34) (end 8.02 -6.66) (layer "F.SilkS") (width 0.12) (tstamp 900e54ac-330f-43f3-9551-03091c717781))
  (fp_line (start -6.35 -8.89) (end -3.81 -8.89) (layer "F.SilkS") (width 0.12) (tstamp e0840473-35db-4fb2-9daa-a5797481a384))
  (pad "1" thru_hole circle (at -5.3 4.35) (size 2 2) (drill 1.1) (layers *.Cu *.Mask) (tstamp 7ff9ba60-8210-4de3-a719-42fa33825999))
  (pad "1" thru_hole circle (at -5.3 -4.35) (size 2 2) (drill 1.1) (layers *.Cu *.Mask) (tstamp 99dfc74b-21a8-4fac-a33b-3bfd82550dc0))
  (pad "2" thru_hole circle (at 0 -4.35) (size 2 2) (drill 1.1) (layers *.Cu *.Mask) (tstamp c56a3ce8-80b1-41e7-88c9-d504fecb41b4))
  (pad "2" thru_hole circle (at 0 4.35) (size 2 2) (drill 1.1) (layers *.Cu *.Mask) (tstamp e98aa069-b4d7-4ef7-8631-db8798dff242))
  (pad "3" thru_hole circle (at 5.3 -4.35) (size 2 2) (drill 1.1) (layers *.Cu *.Mask) (tstamp 5696b62e-f9d5-491d-b030-c9cb45f6028a))
  (pad "3" thru_hole circle (at 5.3 4.35) (size 2 2) (drill 1.1) (layers *.Cu *.Mask) (tstamp 63359286-beaf-4c54-b415-0bbfefb3f9c6))
  (model "${INT_PACKAGE_DIR}/810_connectors_clable_to_Board/pxc_1017504_00_TDPT-2-5-3-SP-5-08_3D.stp"
    (offset (xyz -8 -10 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
