(footprint "bourns_SRR3818_3.8x3.8_mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.1 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp a0b4a016-0a36-45a8-8614-6faff2372d19)
  )
  (fp_text value "bourns_SRR3818_3.8x3.8_mm" (at -6.7 -17.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2e898c51-ea3a-4e2f-95c4-c1df9ae7c78c)
  )
  (fp_text user "${REFERENCE}" (at 0 4.4 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c01cfc67-b6f6-4ed1-bc36-cbfec8b834be)
  )
  (fp_rect (start -1.9 -0.5) (end -1.9 0.5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 9d0c7d70-5bfa-4aae-a38b-59ae934a2eb2))
  (fp_rect (start 1.9 -0.5) (end 1.9 0.5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp a055a4bd-1d9b-47f4-9618-23db4289a6d5))
  (fp_rect (start -2.3 -2.3) (end 2.3 2.3)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.CrtYd") (tstamp cd70f7eb-5ecd-4384-8a24-7f97d5a5191a))
  (pad "1" smd rect (at 0 -1.35) (size 4.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a4b1eca4-b825-4292-9f2f-80d54c736838))
  (pad "2" smd rect (at 0 1.35) (size 4.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp dafb147e-027b-4c13-8fde-2f035bfe9e6e))
  (model ":KICED_3DMODELS_DIR:021_inductor/SRR3818A.stp"
    (offset (xyz 0 0 1.8))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
