(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "MAX4684ETB+T " (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -10.16 15.24 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MAX4684ETB+T " (at -1.27 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:TDFN-10-1EP_2x3mm_P0.5mm_EP0.9x2mm" (at 1.27 27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX4684-MAX4685.pdf" (at 1.27 30.48 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Analogue Switch ICs 0.5Ohm Low-Voltage, Dual SPDT Analog Switches " (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX4684ETB+T _0_1"
      (rectangle (start -10.16 13.97) (end 10.16 -13.97)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center -2.54 -2.54) (radius 0.4016)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center -2.54 6.35) (radius 0.4016)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -12.7)
          (xy -6.35 -12.7)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -8.89)
          (xy -6.35 -8.89)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.81 -2.54)
          (xy -2.54 -2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.81 6.35)
          (xy -2.54 6.35)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -2.54)
          (xy 4.445 -0.508)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 6.35)
          (xy 4.445 8.382)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -5.08)
          (xy 3.81 -5.08)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy 3.81 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 3.81)
          (xy 3.81 3.81)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 8.89)
          (xy 3.81 8.89)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -5.08)
          (xy 4.064 -4.699)
          (xy 4.318 -5.08)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 0)
          (xy 4.064 -0.381)
          (xy 4.318 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 3.81)
          (xy 4.064 4.191)
          (xy 4.318 3.81)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 8.89)
          (xy 4.064 8.509)
          (xy 4.318 8.89)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -11.684)
          (xy -5.08 -13.716)
          (xy -3.302 -12.7)
          (xy -5.08 -11.684)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 -7.874)
          (xy -5.08 -9.906)
          (xy -3.302 -8.89)
          (xy -5.08 -7.874)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "MAX4684ETB+T _1_1"
      (polyline
        (pts
          (xy -3.302 -12.7)
          (xy 1.27 -12.7)
          (xy 1.27 -1.524)
        )
        (stroke (width 0) (type dash))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.302 -8.89)
          (xy -1.27 -8.89)
          (xy -1.27 6.604)
        )
        (stroke (width 0) (type dash))
        (fill (type none))
      )
      (pin power_in line (at 7.62 16.51 270) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
        (name "NO2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 3.81 180) (length 2.54)
        (name "NO1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 6.35 0) (length 2.54)
        (name "COM1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -8.89 0) (length 2.54)
        (name "IN1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 8.89 180) (length 2.54)
        (name "NC1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -16.51 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 0 180) (length 2.54)
        (name "NC2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 2.54)
        (name "IN2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
        (name "COM2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
