(footprint "HTSSOP48" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -10.45 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 6cc550cb-bba4-411d-8dd4-3f57cf5157fe)
  )
  (fp_text value "HTSSOP48" (at 0 -8.95 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6d48104c-509a-41a4-9a7d-a363ead13db3)
  )
  (fp_text user "${REFERENCE}" (at 0 -7.45 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6907d769-1a97-4e1b-8230-9649c67221f7)
  )
  (fp_rect (start -3.05 -6.25) (end 3.05 6.25)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp d5326d41-d1cf-464e-a792-c38515fb5b99))
  (pad "1" smd rect (at -3.65 -5.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c35b17a1-21f5-49cf-aa45-af33682a0d34))
  (pad "2" smd rect (at -3.65 -5.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 10c14217-16ec-465b-b649-94122392dfaf))
  (pad "3" smd rect (at -3.65 -4.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 835fb729-755f-4345-9550-87a8758bb25c))
  (pad "4" smd rect (at -3.65 -4.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 172ce7c1-1b3a-47d1-a65c-d88888bdc902))
  (pad "5" smd rect (at -3.65 -3.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a5cfb18f-d028-42f4-a4f1-030c351cdcbe))
  (pad "6" smd rect (at -3.65 -3.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6e922013-9d32-43e4-a4e0-007dff8b24c7))
  (pad "7" smd rect (at -3.65 -2.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 5f065316-3494-46be-b21e-07af84825837))
  (pad "8" smd rect (at -3.65 -2.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 63762e2f-8a1c-42f7-90e9-096ca7969d01))
  (pad "9" smd rect (at -3.65 -1.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 40427da0-27c6-4a35-8735-6d464a9090ca))
  (pad "10" smd rect (at -3.65 -1.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c1404900-18fc-42dd-a421-834d752c9db3))
  (pad "11" smd rect (at -3.65 -0.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 9af9993a-f000-4aff-85c7-30392258e468))
  (pad "12" smd rect (at -3.65 -0.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp cc103ad0-57c4-4c09-bb08-10ba97342050))
  (pad "13" smd rect (at -3.65 0.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 493ee647-8674-48de-bb0d-a44b78c1b7bd))
  (pad "14" smd rect (at -3.65 0.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a85dc2a4-848d-4b26-853a-5b53da785ce1))
  (pad "15" smd rect (at -3.65 1.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 0ce28c8d-345a-48f1-90ea-e716fe31850d))
  (pad "16" smd rect (at -3.65 1.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 1da542e6-6630-421e-a049-47211c6b61cf))
  (pad "17" smd rect (at -3.65 2.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp cf1d00da-51e6-4638-a6f1-17c77dcfc4ea))
  (pad "18" smd rect (at -3.65 2.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp fcd6b3fb-9449-496d-a8c6-93f2bc4d4485))
  (pad "19" smd rect (at -3.65 3.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 2af63dc4-22b2-4473-a491-9e8dd588a5f3))
  (pad "20" smd rect (at -3.65 3.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp f2f485f0-b5f5-4d91-b724-c842ec86f910))
  (pad "21" smd rect (at -3.65 4.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp b9c8ee9f-8a41-48c6-bf7d-4a50745ba51b))
  (pad "22" smd rect (at -3.65 4.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 17fb5cc5-c7af-4625-80da-9fa13729d7f2))
  (pad "23" smd rect (at -3.65 5.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 58fb0c52-e285-4838-b02c-736274db72b1))
  (pad "24" smd rect (at -3.65 5.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 12a85f7b-6b57-4e3e-be24-10bd74c56d4f))
  (pad "25" smd rect (at 3.65 5.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp b853e668-b64f-4d18-965c-5132e2b25884))
  (pad "26" smd rect (at 3.65 5.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a7110cce-b982-4922-83e3-b7fa4ba7887b))
  (pad "27" smd rect (at 3.65 4.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 935f5556-24ce-4a85-bf9a-0881129e0ca7))
  (pad "28" smd rect (at 3.65 4.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 315a5ec9-f84f-4d62-8f02-53c472cae386))
  (pad "29" smd rect (at 3.65 3.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 95887554-4300-483a-b273-93e543b35074))
  (pad "30" smd rect (at 3.65 3.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 4d542934-9e2d-4919-a8ec-513eff5906e4))
  (pad "31" smd rect (at 3.65 2.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 48cb1944-f90c-4fc5-b55b-1bb0bfa0604e))
  (pad "32" smd rect (at 3.65 2.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 72155e00-4427-4b54-b022-0e16c1e99e21))
  (pad "33" smd rect (at 3.65 1.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 66b15c25-d3e0-439c-ba3b-0ca2010a5cb2))
  (pad "34" smd rect (at 3.65 1.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 521a4404-9c14-4dca-a6fe-dbce997448a3))
  (pad "35" smd rect (at 3.65 0.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp d1289e91-f3d8-4fee-8a68-142ea467b920))
  (pad "36" smd rect (at 3.65 0.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a91c7da3-f823-4393-b5e3-45bce750f42b))
  (pad "37" smd rect (at 3.65 -0.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp bff23b0d-0064-4516-8b62-f1ab7b48a8b6))
  (pad "38" smd rect (at 3.65 -0.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 029fcf1f-a296-4e68-aca4-546c31fb1e5d))
  (pad "39" smd rect (at 3.65 -1.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 97d249a6-1157-4665-b82a-430b1c8d41ea))
  (pad "40" smd rect (at 3.65 -1.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 53a35033-fbc4-45a6-9e97-5a427ff5ff9c))
  (pad "41" smd rect (at 3.65 -2.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 04ac610d-1775-4cae-a845-c65003f55338))
  (pad "42" smd rect (at 3.65 -2.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 019ee1e4-b163-439f-8cfb-f3ef250f17cf))
  (pad "43" smd rect (at 3.65 -3.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 27f49cf9-b9da-4d05-9474-fec5bf273ec6))
  (pad "44" smd rect (at 3.65 -3.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 61e5fe5e-2958-454c-944b-5be3e5404fbc))
  (pad "45" smd rect (at 3.65 -4.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp fc383260-74b5-4b29-ba49-48e92fec02bb))
  (pad "46" smd rect (at 3.65 -4.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 8dbd106d-aae1-4e43-97e7-73ce027c694b))
  (pad "47" smd rect (at 3.65 -5.25) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp d36e779a-f16a-4fa3-924d-514dcc5e6c6d))
  (pad "48" smd rect (at 3.65 -5.75) (size 1.45 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 491ce5fd-a8f1-4d8c-b67f-a3316ee31c63))
  (pad "PAD" smd rect (at 0 0) (size 3.9 6.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp f8693481-5387-41c9-81e5-b5c1468578da))
  (model ":KICAD7_3DMODEL_DIR:Package_SO.3dshapes/TSSOP-48_6.1x12.5mm_P0.5mm.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
