(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "LAN9253_R4X"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 29.464 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Value" "LAN9253/R4X"
			(at -30.226 -31.242 0)
			(effects
				(font
					(size 1.524 1.524)
				)
			)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP6x6mm_ThermalVias"
			(at 0 51.308 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "LAN9253/R4X"
			(at 0 53.848 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at -66.04 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "ki_keywords" "LAN9253/R4X"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "QFN64_R4X_MCH QFN64_R4X_MCH-M QFN64_R4X_MCH-L"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "LAN9253_R4X_1_1"
			(rectangle
				(start -38.1 27.94)
				(end 38.1 -29.21)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy 0 -7.62) (xy 38.1 -7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 38.1 13.97) (xy -38.1 13.97)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -38.1 -3.81) (xy 0 -3.81) (xy 0 13.97)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -29.21) (xy -38.1 -29.21)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(text "INT PORT1"
				(at 15.748 3.556 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(text "INT PORT2"
				(at 15.24 -19.05 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(text "OCS"
				(at -14.224 5.08 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(text "OTHER \nSIGNALS"
				(at -13.462 -12.954 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(text "POWER"
				(at -35.306 20.574 900)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(pin input line
				(at -45.72 7.62 0)
				(length 7.62)
				(name "OSCI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -45.72 -15.24 0)
				(length 7.62)
				(name "RST#"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 7.62)
				(name "VDDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -45.72 3.81 0)
				(length 7.62)
				(name "OSCO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 7.62)
				(name "VDDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 35.56 270)
				(length 7.62)
				(name "VDDCR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -45.72 11.43 0)
				(length 7.62)
				(name "OSCVDD12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 7.62)
				(name "VDDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 7.62)
				(name "VDDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 17.78 35.56 270)
				(length 7.62)
				(name "VDDCR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at -45.72 0 0)
				(length 7.62)
				(name "OSCVSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -45.72 -26.67 0)
				(length 7.62)
				(name "TESTMODE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -45.72 -19.05 0)
				(length 7.62)
				(name "IRQ/LATCH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 7.62)
				(name "VDDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -12.7 35.56 270)
				(length 7.62)
				(name "VDD33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -30.48 35.56 270)
				(length 7.62)
				(name "VDD33TXRX1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at 45.72 7.62 180)
				(length 7.62)
				(name "TNXA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at 45.72 5.08 180)
				(length 7.62)
				(name "TXPA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at 45.72 2.54 180)
				(length 7.62)
				(name "RXNA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at 45.72 0 180)
				(length 7.62)
				(name "RXPA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 25.4 35.56 270)
				(length 7.62)
				(name "VDD12TX1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at -45.72 -11.43 0)
				(length 7.62)
				(name "RBIAS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -20.32 35.56 270)
				(length 7.62)
				(name "VDD33BIAS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 27.94 35.56 270)
				(length 7.62)
				(name "VDD12TX2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 12.7 35.56 270)
				(length 7.62)
				(name "VDDCR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at 45.72 -22.86 180)
				(length 7.62)
				(name "RXPB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at 45.72 -20.32 180)
				(length 7.62)
				(name "RXNB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at 45.72 -17.78 180)
				(length 7.62)
				(name "TXPB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at 45.72 -15.24 180)
				(length 7.62)
				(name "TXNB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -27.94 35.56 270)
				(length 7.62)
				(name "VDD33TXRX2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 35.56 35.56 270)
				(length 7.62)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin unspecified line
				(at -45.72 -7.62 0)
				(length 7.62)
				(name "REG_EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -45.72 -22.86 0)
				(length 7.62)
				(name "CLK_25/CLK_25_EN/XTAL_MODE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "LAN9253_R4X_2_1"
			(rectangle
				(start -53.34 10.16)
				(end 50.8 -10.16)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy -53.34 0) (xy 50.8 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 10.16) (xy 0 -10.16)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(text "Clock Sync/Latch \n      (OUT/IN)"
				(at -12.7 5.08 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(text "I2C\nEEPROM"
				(at 20.32 -4.826 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(text "MODE"
				(at 5.334 3.556 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(text "Status"
				(at -10.414 -3.302 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(pin bidirectional line
				(at -60.96 7.62 0)
				(length 7.62)
				(name "SYNC1/LATCH1/PME"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -60.96 3.81 0)
				(length 7.62)
				(name "SYNC0/LATCH0/PME"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -3.81 180)
				(length 7.62)
				(name "EESDA/TMS/EE_EMUL1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 -7.62 180)
				(length 7.62)
				(name "EESCL/TCK/EE_EMUL2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -60.96 -7.62 0)
				(length 7.62)
				(name "RUNLED/STATE_RUNLED/E2PSIZE/EE_EMUL0/LEDPOL3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 3.81 180)
				(length 7.62)
				(name "LINKACTLED1/TDI/CHIP_MODE1/LEDPOL1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 58.42 7.62 180)
				(length 7.62)
				(name "LINKACTLED0/TDO/CHIP_MODE0/100FD_A/LEDPOL0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -60.96 -3.81 0)
				(length 7.62)
				(name "ERRLED/PME/100FD_B/LEDPOL4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "LAN9253_R4X_3_1"
			(rectangle
				(start -45.72 -11.43)
				(end 0 -24.13)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -45.72 19.05)
				(end 44.45 -24.13)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start -7.62 19.05)
				(end -45.72 -6.35)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(text "DNP"
				(at -27.0897 -13.8086 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(text "SPI"
				(at -27.432 -3.048 0)
				(effects
					(font
						(size 1.524 1.524)
						(thickness 0.3048)
						(bold yes)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -20.32 0)
				(length 7.62)
				(name "WAIT_ACK/PME/LATCH0//EE_EMUL_SPI3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 6.35 0)
				(length 7.62)
				(name "D2/AD2/SOF/SIO2/EE_EMUL_SPI0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 8.89 0)
				(length 7.62)
				(name "D1/AD1/EOF/SO/SIO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 -3.81 180)
				(length 7.62)
				(name "D14/AD14/DIGIO8/GPI8/GPO8/MII_TXD3/TX_SHIFT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 -1.27 180)
				(length 7.62)
				(name "D13/AD13/DIGIO7/GPI7/GPO7/MII_TXD2/TX_SHIFT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 11.43 0)
				(length 7.62)
				(name "D0/AD0/WD_STATE/SI/SIO0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 16.51 0)
				(length 7.62)
				(name "D9/AD9/LATCH_IN/SCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 13.97 180)
				(length 7.62)
				(name "D12/AD12/DIGIO6/GPI6/GPO6/MII_TXD1/100FD_B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 11.43 180)
				(length 7.62)
				(name "D11/AD11/DIGIO5/GPI5/GPO5/MII_TXD0/100FD_A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 8.89 180)
				(length 7.62)
				(name "D10/AD10/DIGIO4/GPI4/GPO4/MII_TXEN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 -17.78 0)
				(length 7.62)
				(name "A1/ALELO/OE_EXT/MII_CLK25//EE_EMUL_SPI2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 -11.43 180)
				(length 7.62)
				(name "A3/BE0/DIGIO11/GPI11/GPO11/MII_RXDV"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 -13.97 180)
				(length 7.62)
				(name "A4/BE1/DIGIO12/GPI12/GPO12/MII_RXD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 -16.51 180)
				(length 7.62)
				(name "CS/DIGIO13/GPI13/GPO13/MII_RXD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 -8.89 180)
				(length 7.62)
				(name "A2/ALEHI/DIGIO10/GPI10/GPO10/LINKACTLED2/EE_EMUL_ALELO_POL/MII_LINKPOL/LEDPOL2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 -19.05 180)
				(length 7.62)
				(name "WR/ENB/DIGIO14/GPI14/GPO14/MII_RXD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 -21.59 180)
				(length 7.62)
				(name "RD/RD_WR/DIGIO15/GPI15/GPO15/MII_RXD3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 -6.35 180)
				(length 7.62)
				(name "A0/D15/AD15/DIGIO9/GPI9/GPO9/MII_RXER"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 3.81 0)
				(length 7.62)
				(name "D3/AD3/WD_TRIG/SIO3/EE_EMUL_SPI1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 16.51 180)
				(length 7.62)
				(name "D6/AD6/DIGIO0/GPI0/GPO0/MII_RXCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 1.27 180)
				(length 7.62)
				(name "D7/AD7/DIGIO1/GPI1/GPO1/MII_MDC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 3.81 180)
				(length 7.62)
				(name "D8/AD8/DIGIO2/GPI2/GPO2/MII_MDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 52.07 6.35 180)
				(length 7.62)
				(name "D4/AD4/DIGIO3/GPI3/GPO3/MII_LINK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -53.34 13.97 0)
				(length 7.62)
				(name "D5/AD5/OUTVALID/SCS#"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
)
