(module BD9F800MUX (layer F.Cu) (tedit 5F4FB4C6)
  (descr "4.5V to 28V Input, 8.0A Integrated MOSFET Single Synchronous Buck DC/DC Converter")
  (tags "dcdc buck rohm converter")
  (zone_connect 2)
  (attr smd)
  (fp_text reference U1 (at 0.07 3 -180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value BD9F800MUX (at 0 3 -180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.Fab) (width 0.001))
  (fp_line (start 1.75 -1.75) (end 1.75 1.75) (layer F.Fab) (width 0.001))
  (fp_line (start 1.75 1.75) (end -1.75 1.75) (layer F.Fab) (width 0.001))
  (fp_line (start -1.75 1.75) (end -1.75 -1.75) (layer F.Fab) (width 0.001))
  (fp_line (start 1.75 0) (end -1.75 0) (layer F.Fab) (width 0.001))
  (fp_line (start -1.75 -1.15) (end -1.75 -1.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.75 -1.75) (end -1.45 -1.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.45 -1.75) (end 1.75 -1.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.75 -1.75) (end 1.75 -1.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.75 1.75) (end -1.45 1.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.45 1.75) (end 1.75 1.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -1.75) (end 0 -0.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.75 0) (end 1.75 0) (layer F.SilkS) (width 0.12))
  (fp_circle (center 2 -2.15) (end 2.05 -2.15) (layer F.SilkS) (width 0.12))
  (pad 1 smd roundrect (at 1.25 -2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 2 smd roundrect (at 0.75 -2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 3 smd roundrect (at 0.25 -2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 4 smd roundrect (at -0.25 -2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 5 smd roundrect (at -0.75 -2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 6 smd roundrect (at -1.25 -2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 7 smd roundrect (at -2.05 -0.94) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 11 smd roundrect (at 2.05 -0.94) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 8 smd oval (at 0 -0.325) (size 3.2 0.4) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 9 smd oval (at 0 0.325 180) (size 3.2 0.4) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 10 smd rect (at 0 1.238) (size 3.2 0.725) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 8 smd roundrect (at 2.05 -0.325) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 9 smd roundrect (at 2.05 0.325) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 9 smd roundrect (at -2.05 0.325) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 8 smd roundrect (at -2.05 -0.325) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at -2.05 0.9905) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at -2.05 1.4855) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at 1.25 2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at 0.75 2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at 0.25 2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at -1.25 2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at -0.75 2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at -0.25 2.05) (size 0.23 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at 2.05 1.4855) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (pad 10 smd roundrect (at 2.05 0.99) (size 1.4 0.23) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
    (zone_connect 2))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_VQFN-RGR-20-1EP_3.5x3.5mm_Pitch0.5mm.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
