(footprint "PV-T22-38E" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "H**" (at -26 -16 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp f2426c7b-2d22-4715-b65f-62cfd7bc8ea4)
  )
  (fp_text value "PV-T22-38E" (at 0 -16 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 81760948-6591-4f54-892a-19fa4b702132)
  )
  (fp_text user "${REFERENCE}" (at 19 -16 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1d64daa6-2dda-469a-a68a-ec7e10f0bf75)
  )
  (fp_rect (start -27.55 -14.5) (end 27.55 3)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.SilkS") (tstamp 4a0c9218-3689-46b4-ade2-8dc65de9dd4d))
  (fp_rect (start -28.05 -15) (end 28.05 3)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.CrtYd") (tstamp de194060-afa1-4d61-b6be-76033db2d267))
  (pad "" np_thru_hole circle (at -20.55 0) (size 3.8 3.8) (drill 2.7) (layers "F&B.Cu" "*.Mask") (tstamp 2b6eae74-0cbe-4c9a-ba9e-3303d1687776))
  (pad "" np_thru_hole circle (at 20.55 0) (size 3.8 3.8) (drill 2.7) (layers "F&B.Cu" "*.Mask") (tstamp 186e3694-7abc-4bab-a4e7-79d68c504e7e))
)
