(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -8.89 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LTC2935ITS8-2" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (at 3.81 19.05 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2935fa.pdf" (at 1.27 21.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "_0_1"
      (rectangle (start -8.89 10.16) (end 8.89 -11.43)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "_1_1"
      (pin input line (at -11.43 7.62 0) (length 2.54)
        (name "S2" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 5.08 0) (length 2.54)
        (name "S1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 2.54 0) (length 2.54)
        (name "S0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -13.97 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 7.62 180) (length 2.54)
        (name "~{PFO}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -8.89 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 -8.89 0) (length 2.54)
        (name "~{MR}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LTC2935ITS8-2" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -8.89 12.7 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "LTC2935ITS8-2" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (at 0 24.13 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2935fa.pdf" (at 1.27 26.67 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LTC2935ITS8-2_0_1"
      (rectangle (start -8.89 11.43) (end 8.89 -11.43)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "LTC2935ITS8-2_1_1"
      (pin input line (at -11.43 8.89 0) (length 2.54)
        (name "S2" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 6.35 0) (length 2.54)
        (name "S1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 3.81 0) (length 2.54)
        (name "S0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -13.97 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 8.89 180) (length 2.54)
        (name "~{PFO}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -8.89 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -8.89 0) (length 2.54)
        (name "~{MR}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 13.97 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LTC2935ITS8-3" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -8.89 12.7 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "LTC2935ITS8-3" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-8" (at 0 25.4 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2935fa.pdf" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LTC2935ITS8-3_0_1"
      (rectangle (start -8.89 11.43) (end 8.89 -11.43)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "LTC2935ITS8-3_1_1"
      (pin input line (at -11.43 8.89 0) (length 2.54)
        (name "S2" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 6.35 0) (length 2.54)
        (name "S1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 3.81 0) (length 2.54)
        (name "S0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -13.97 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 8.89 180) (length 2.54)
        (name "~{PFO}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -8.89 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -8.89 0) (length 2.54)
        (name "~{MR}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 13.97 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
