(footprint "CL-SB-22A"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -7.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "eac1c77c-4c07-493d-be3a-ceb32c22bed5")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "CL-SB-22A"
		(at 0 -11.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "2c889706-8d46-42bc-b737-ebd92981454d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "580f1446-9b4f-4f5f-b8c0-4e4271632897")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8143201e-5e1c-41be-a62b-bc8f5bdb3707")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7727bb99-42c6-478a-93cd-ea59300f7e39")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -4.25 -2.5)
		(end 4.25 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "8f9a3802-f8f1-486a-8abc-83f09b576483")
	)
	(fp_rect
		(start -4.25 -2.5)
		(end 4.25 2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "d95ab8b0-add9-4cd8-ac49-9471dfab599a")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -10 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "365f0f8d-0a58-4a5b-8698-e06076a1eb77")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.5 1.4)
		(size 1.2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "1b1c5613-1954-42f7-a60b-3ff44ce040fc")
	)
	(pad "2" smd roundrect
		(at 0 1.4)
		(size 1.2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "de453e7d-f649-4b96-83e3-5f69abbeea3a")
	)
	(pad "3" smd roundrect
		(at 2.5 1.4)
		(size 1.2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "7cfba159-15da-4c02-b12d-cdbc6caeac3c")
	)
	(pad "4" smd roundrect
		(at 2.5 -1.4)
		(size 1.2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "d8926fdc-39db-4a09-ac62-3df35ddb7a1e")
	)
	(pad "5" smd roundrect
		(at 0 -1.4)
		(size 1.2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "2d8b04be-54e4-45a3-aea9-b2a2974e3920")
	)
	(pad "6" smd roundrect
		(at -2.5 -1.4)
		(size 1.2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "85d00b88-4c8d-4a62-941b-181cb2b0e155")
	)
	(model "/home/key/git/KicED/packages/870_button_smd/CL-SB-22A-12T.stp"
		(offset
			(xyz 0 0 3)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
