(footprint "KXOB25" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -9 -4.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 80c97db3-3161-42b0-a9a8-3e6f557c0ce9)
  )
  (fp_text value "KXOB25" (at -1 -0.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e4e137d9-64ef-4c57-b4cf-6cc9917494ad)
  )
  (fp_text user "+" (at -8.5 0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 4f5cb8e6-15af-468d-901d-0f5ad0c6c43f)
  )
  (fp_text user "-" (at 7.5 0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 74c1f32a-ece8-425b-95e5-4e346e38167d)
  )
  (fp_text user "${REFERENCE}" (at -1 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f27ed1b4-7bb1-4208-aaf8-5c04b809e055)
  )
  (fp_line (start -11 -3.4) (end 11 -3.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 946cd56a-8008-40eb-a645-3585fadaa7cd))
  (fp_line (start -11 3.4) (end 11 3.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 4c186e90-1623-495f-ae2c-86b9a115b861))
  (fp_rect (start -11.5 -3.5) (end 11.5 3.5)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp d3bcd769-310f-4273-8a5a-5d3f18a0d6eb))
  (pad "1" smd roundrect (at -10 0) (size 2 6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp f6a86cee-b17d-4ffc-94a0-b31f15fd0239))
  (pad "2" smd roundrect (at 10 0) (size 2 6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 9d15063c-ec7c-449a-8fde-c274883afca8))
)
