(footprint "amphenol_BergStak_header_2Rows-50Pins_0.4mm_1.5mmStack-Height" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (clearance 0.08)
  (attr smd)
  (fp_text reference "REF**" (at -17.6 -0.2 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8bdb4081-d0cb-4bc7-b525-7d5ae3a0d185)
  )
  (fp_text value "amphenol_BergStak_header_2Rows-50Pins_0.4mm_1.5mmStack-Height" (at 0 5.6) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 61b36eee-8fb1-4c0a-aa50-8dc9552dff40)
  )
  (fp_rect (start -6.01 -1.935) (end 6.01 1.935)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp c72982b9-ab39-49bd-9ec0-66d2f9121f30))
  (fp_circle (center -5.5 1.4) (end -5.3 1.4)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.SilkS") (tstamp aebbadb9-85f4-4528-8856-e2906134e665))
  (fp_rect (start -5.81 -1.735) (end 5.81 1.735)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.CrtYd") (tstamp 46e78805-8d2e-44af-8fb1-6ad5f3da17ed))
  (pad "1" smd rect (at -4.8 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp f351d3be-a4b1-4400-824d-44c652a18c7c))
  (pad "2" smd rect (at -4.8 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 2f111214-ecd2-4e92-a513-6f414e58d9e1))
  (pad "3" smd rect (at -4.4 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 762834b2-22d1-4438-8e5a-9d161ba51489))
  (pad "4" smd rect (at -4.4 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c1956b9e-0c7f-4b2f-884d-28a276332690))
  (pad "5" smd rect (at -4 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp cf4bc76c-6814-4d19-8afb-f1d4044290ba))
  (pad "6" smd rect (at -4 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 3bcac6b4-ad44-4c8a-8200-87f6b9b0a6b1))
  (pad "7" smd rect (at -3.6 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6c63062e-9bb8-4186-ac00-bdcccc1977e9))
  (pad "8" smd rect (at -3.6 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 579be023-d295-4911-a0c8-0641ff9c110a))
  (pad "9" smd rect (at -3.2 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 7129ab5d-e9e5-463c-bad3-01a6227b6452))
  (pad "10" smd rect (at -3.2 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp f919ebf3-7484-4d59-80ef-13a9b64d142f))
  (pad "11" smd rect (at -2.8 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp f2ec2982-38a9-4b5c-b956-a37659e882bc))
  (pad "12" smd rect (at -2.8 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c04b2680-f3af-415c-98a2-4565d87f9be0))
  (pad "13" smd rect (at -2.4 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 72016797-118f-485c-8ae1-399cb607567b))
  (pad "14" smd rect (at -2.4 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 37b3df71-aa99-4705-bfda-70f6a500b3b3))
  (pad "15" smd rect (at -2 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6e716aec-bc39-4ffd-a52c-43ea548db548))
  (pad "16" smd rect (at -2 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 91787181-c3c1-4881-b42d-1ffaebdcb64d))
  (pad "17" smd rect (at -1.6 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp ca4e5b47-106f-4cbd-9fd3-407afaedeb98))
  (pad "18" smd rect (at -1.6 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 30204b43-d603-40ef-a678-7447ff0a3bdb))
  (pad "19" smd rect (at -1.2 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 25baa327-c0ae-4d49-a0b7-20a7787ad3fd))
  (pad "20" smd rect (at -1.2 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 5a75fc7d-87d4-4280-9bc4-f46579c5b71f))
  (pad "21" smd rect (at -0.8 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 218767b0-7c06-44b7-a3ee-374f4bb75dad))
  (pad "22" smd rect (at -0.8 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 9ce0a148-8dee-4dcd-9183-63c735ab9bd0))
  (pad "23" smd rect (at -0.4 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 8f2eed0f-fb67-4728-9e80-d0ca5c72b01e))
  (pad "24" smd rect (at -0.4 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 3664cd6c-0e81-4b8f-a3b8-87e5c0eaa82d))
  (pad "25" smd rect (at 0 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a4cda7d6-6a8e-4c70-ad55-09400ba16883))
  (pad "26" smd rect (at 0 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp f500e994-b859-47f6-b60f-c2c395aa6cb2))
  (pad "27" smd rect (at 0.4 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp fe10caf9-126d-4e38-84b9-5b74f894bc31))
  (pad "28" smd rect (at 0.4 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp d39f88ab-4843-4548-b0bb-6db15e1d4dc6))
  (pad "29" smd rect (at 0.8 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 39ee43ad-5008-4eeb-8e0e-7f3d1943acdb))
  (pad "30" smd rect (at 0.8 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp cc222e2b-894f-4351-bd17-523845927a62))
  (pad "31" smd rect (at 1.2 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp ed9913c8-7a21-4eb6-a8e4-a0fae0fc6fe8))
  (pad "32" smd rect (at 1.2 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 1a62c73e-9fd3-4c17-a16f-044921552497))
  (pad "33" smd rect (at 1.6 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp ae5f10cd-a7a0-43bd-8662-5165c451a2d0))
  (pad "34" smd rect (at 1.6 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a159c6c8-347c-406e-9653-57da00f151ee))
  (pad "35" smd rect (at 2 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6644b590-2454-4fe7-85dc-ca9d0c7f32f2))
  (pad "36" smd rect (at 2 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp cc74feda-0f12-4027-addd-9ac73c2d5ef2))
  (pad "37" smd rect (at 2.4 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 8f4d7161-6c54-45bb-a5db-a233195b3492))
  (pad "38" smd rect (at 2.4 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a7365f90-96fc-4874-9c23-87318598a6d8))
  (pad "39" smd rect (at 2.8 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 5dca1b24-7626-4ca5-818f-112edbe0289c))
  (pad "40" smd rect (at 2.8 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6363ecd3-354e-4ada-814b-ad1bc0501d4f))
  (pad "41" smd rect (at 3.2 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 59932a1b-195f-4f98-9839-36915c0ba97c))
  (pad "42" smd rect (at 3.2 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 316ad9bb-515d-475a-bba9-ab8c4ead42d2))
  (pad "43" smd rect (at 3.6 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp b544024f-4821-4d5a-9f26-feadf25c1f79))
  (pad "44" smd rect (at 3.6 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 22862e73-1862-4db8-9b4b-a3fb0d6e80e5))
  (pad "45" smd rect (at 4 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 303b0ccf-5ffd-4a22-9de6-2eb8d8cc4f74))
  (pad "46" smd rect (at 4 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 93f60649-c3c0-4c62-8228-7fc54788c4c0))
  (pad "47" smd rect (at 4.4 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 681ee100-381e-4a46-a9ca-47c6d9642d4b))
  (pad "48" smd rect (at 4.4 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp d07a56a8-099c-48a3-9bcb-bbe441017807))
  (pad "49" smd rect (at 4.8 1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6dc72316-c117-40da-bd60-5c15f9ff56b7))
  (pad "50" smd rect (at 4.8 -1.355) (size 0.23 0.66) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c5718a7f-6f71-4476-83a5-6eabbb585381))
  (model "/home/key/git/brayn/02_hardware/KicED/packages/811_connectors_board_to_board/10164228-0501a1rlf.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
