(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "PEL12D-4225S-S1024" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 10.16 15.24 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "PEL12D-4225S-S1024" (at 10.16 12.7 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "PEL12D4225SS1024" (at 21.59 -87.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://www.arrow.com/en/products/pel12d-4225s-s1024/bourns" (at 21.59 -187.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Man" "Bourns" (at 21.59 -487.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Man_No" "PEL12D-4225S-S1024" (at 21.59 -587.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Disti" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Disti_No" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PEL12D - 12 mm Encoder with Switch and Illuminated Shaft" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PEL12D-4225S-S1024_1_1"
      (rectangle (start -6.35 7.62) (end 6.35 -6.35)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin passive line (at 3.81 12.7 270) (length 5.08)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 1.27 12.7 270) (length 5.08)
        (name "+_1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -1.27 12.7 270) (length 5.08)
        (name "+_2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -3.81 12.7 270) (length 5.08)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -11.43 90) (length 5.08)
        (name "CCW" (effects (font (size 1.27 1.27))))
        (number "A1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -11.43 90) (length 5.08)
        (name "CW" (effects (font (size 1.27 1.27))))
        (number "B1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -11.43 90) (length 5.08)
        (name "WIPER" (effects (font (size 1.27 1.27))))
        (number "C1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 0 180) (length 5.08)
        (name "MH1" (effects (font (size 1.27 1.27))))
        (number "MH1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 0 0) (length 5.08)
        (name "MH2" (effects (font (size 1.27 1.27))))
        (number "MH2" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
