(footprint "2824" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 5.08 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ec1f605e-2e0f-475d-9dc2-f4165fb0f536)
  )
  (fp_text value "2824" (at 0 -5.08 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4a12bfed-45b0-498c-af6e-67b0a60e0065)
  )
  (fp_text user "${REFERENCE}" (at -5.08 5.08 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c94867e7-86e9-40ae-8df5-18ebed567ac5)
  )
  (fp_line (start -2.54 -3.05) (end 2.54 -3.05) (layer "F.SilkS") (width 0.12) (tstamp 355beb19-8d45-4b86-9e5c-31cf40cf3723))
  (fp_line (start -2.54 3.05) (end 2.54 3.05) (layer "F.SilkS") (width 0.12) (tstamp c22fded5-1e13-4f8d-8f85-611121d37d30))
  (pad "1" smd roundrect (at -4.1 0) (size 2.5 6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ca61e469-3fc1-4646-abb7-91a4e7141921))
  (pad "2" smd roundrect (at 4.1 0) (size 2.5 6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a03d1a13-0c93-4099-a61e-9a88e17fec44))
)
