(module USB_Micro_B_Female_10118193-0001LF (layer F.Cu) (tedit 5FCDF6C1)
  (descr http://portal.fciconnect.com/Comergent//fci/drawing/10118193.pdf)
  (attr smd)
  (fp_text reference REF** (at 0 -4.75) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_Micro_B_Female_10118193-0001LF (at 0 4.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 4.014908 2.461848) (end 4.014908 2.841848) (layer F.SilkS) (width 0.1))
  (fp_line (start 4.014908 2.841848) (end 3.644908 2.841848) (layer F.SilkS) (width 0.1))
  (fp_line (start -4.013324 2.84) (end -3.643324 2.84) (layer F.SilkS) (width 0.1))
  (fp_line (start -4.013324 2.46) (end -4.013324 2.84) (layer F.SilkS) (width 0.1))
  (fp_line (start 4.06 -3.22) (end 4.06 -1.75) (layer F.SilkS) (width 0.1))
  (fp_line (start 4.06 -3.22) (end 2.4 -3.22) (layer F.SilkS) (width 0.1))
  (fp_line (start -4.05 -3.21) (end -2.4 -3.21) (layer F.SilkS) (width 0.1))
  (fp_line (start -4.05 -3.2) (end -4.05 -1.75) (layer F.SilkS) (width 0.1))
  (fp_line (start 3.93 2.75) (end 3.93 -2.9) (layer F.Fab) (width 0.1))
  (fp_line (start -3.93 2.75) (end 3.93 2.75) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0.06 1.86) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.93 -2.34) (end -3.37 -2.9) (layer F.Fab) (width 0.1))
  (fp_line (start 3.93 -2.9) (end -3.37 -2.9) (layer F.Fab) (width 0.1))
  (fp_line (start -3.93 2.75) (end -3.93 -2.34) (layer F.Fab) (width 0.1))
  (fp_line (start 4.25 -3.75) (end 4.25 3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.25 -3.75) (end 4.25 -3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.25 3) (end 4.25 3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.25 -3.75) (end -4.25 3) (layer F.CrtYd) (width 0.05))
  (pad 6 smd rect (at 1.2 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.2 0) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 3.2 -2.45) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -3.2 -2.45) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 6 thru_hole oval (at -3.3 0) (size 0.9 1.6) (drill oval 0.5 1.2) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 3.3 0) (size 0.9 1.6) (drill oval 0.5 1.2) (layers *.Cu *.Mask))
  (pad 1 smd rect (at -1.3 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.65 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.3 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.65 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 -2.675) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
)
