(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "unconnected-(Q1-Pad1)")
  (net 2 "unconnected-(Q1-Pad2)")
  (net 3 "Net-(Q1-Pad10)")
  (net 4 "+")

  (footprint "101_FET:PG-HDSOP-22-1" (layer "F.Cu")
    (tedit 62227FA4) (tstamp ad5a1cde-5335-4c03-b19b-9981458dd0a5)
    (at 159.202 91.44)
    (descr "Infineon PG-HDSOP-10-1 (DDPAK), 20.96x6.5x2.3mm, slug up (https://www.infineon.com/cms/en/product/packages/PG-HDSOP/PG-HDSOP-22-1/)")
    (tags "hdsop 10 ddpak")
    (property "Sheetfile" "SSR.kicad_sch")
    (property "Sheetname" "")
    (path "/8872b179-b0ae-447b-885e-81959fca29f8")
    (attr smd)
    (fp_text reference "Q1" (at 0 -7.62) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 01acb040-f423-491c-bd6f-dbe3cfa66fbb)
    )
    (fp_text value "IPDQ60R010S7" (at 0 7.874) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bda02842-2af5-4aca-ab94-73d9965935ff)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 562e243b-bc50-41eb-ac28-d95f58fc99a3)
    )
    (fp_line (start -7.81 6.78) (end 7.81 6.78) (layer "F.SilkS") (width 0.12) (tstamp 248d6cad-d419-40d1-853e-840dcfdd09cc))
    (fp_line (start -10.9 -6.32) (end -7.81 -6.32) (layer "F.SilkS") (width 0.12) (tstamp 410a699a-6a20-4389-9987-c810022bc43e))
    (fp_line (start 7.81 6.78) (end 7.81 -6.78) (layer "F.SilkS") (width 0.12) (tstamp 5a59c885-5ba9-4a18-9885-fbc96b71fc5c))
    (fp_line (start -7.81 -6.78) (end 7.81 -6.78) (layer "F.SilkS") (width 0.12) (tstamp 973d4f2f-6318-45e3-9c02-5d55daa76d0e))
    (fp_line (start -7.81 6.78) (end -7.81 -6.78) (layer "F.SilkS") (width 0.12) (tstamp fea8bc41-b676-4245-bd29-39fd01a19f13))
    (fp_line (start 11.2 -6.92) (end 11.2 6.92) (layer "F.CrtYd") (width 0.05) (tstamp 7e2eccce-9ce1-4e7f-b50a-d03f18caa6f9))
    (fp_line (start -11.2 6.92) (end 11.2 6.92) (layer "F.CrtYd") (width 0.05) (tstamp 8f6d6868-dff9-43b5-862a-c72dce90fb89))
    (fp_line (start -11.2 -6.92) (end 11.2 -6.92) (layer "F.CrtYd") (width 0.05) (tstamp c6c9af58-0eae-4fc7-bbab-c14be098e0d3))
    (fp_line (start -11.2 -6.92) (end -11.2 6.92) (layer "F.CrtYd") (width 0.05) (tstamp deec98b5-7c2a-42cb-91db-aaddf4344ad6))
    (fp_line (start 10.48 -5.328) (end 7.7 -5.328) (layer "F.Fab") (width 0.1) (tstamp 067a4748-f609-4499-b85b-6eef639d260e))
    (fp_line (start -6.7 -6.71) (end -7.7 -5.71) (layer "F.Fab") (width 0.1) (tstamp 09213558-a053-43d2-85d5-284cacc637f8))
    (fp_line (start 7.7 6.096) (end 10.48 6.096) (layer "F.Fab") (width 0.1) (tstamp 0925c15b-d116-46aa-b60d-b67d842573f6))
    (fp_line (start 7.7 -0.375) (end 10.48 -0.375) (layer "F.Fab") (width 0.1) (tstamp 0d20620d-dbd1-4453-87ee-d4b692153ffa))
    (fp_line (start -10.48 -1.905) (end -7.7 -1.905) (layer "F.Fab") (width 0.1) (tstamp 10068d1b-efb5-4106-b587-148c80d95510))
    (fp_line (start -10.48 2.655) (end -7.7 2.655) (layer "F.Fab") (width 0.1) (tstamp 1b87e744-35d9-40a9-a64b-427493b4f0e2))
    (fp_line (start 10.48 1.515) (end 7.7 1.515) (layer "F.Fab") (width 0.1) (tstamp 28bdbffc-37b9-4d55-9ab5-172e04b00bc1))
    (fp_line (start -7.7 -1.515) (end -10.48 -1.515) (layer "F.Fab") (width 0.1) (tstamp 2a77ba96-a89d-4dcb-b57d-14322b867d87))
    (fp_line (start 10.48 -3.048) (end 7.7 -3.048) (layer "F.Fab") (width 0.1) (tstamp 2aa47f17-97ce-48f9-a21c-d5c782e995b7))
    (fp_line (start -7.7 1.905) (end -10.48 1.905) (layer "F.Fab") (width 0.1) (tstamp 2b3b3acf-f92c-47c0-8463-698effa93d68))
    (fp_line (start 10.48 1.905) (end 10.48 2.655) (layer "F.Fab") (width 0.1) (tstamp 32692498-db6b-49e5-bf30-3dd11d595055))
    (fp_line (start -7.7 5.334) (end -10.48 5.334) (layer "F.Fab") (width 0.1) (tstamp 334b527a-d94a-4eb4-a5a5-cc8fd0f35ff8))
    (fp_line (start -7.3 -6.075) (end -10.48 -6.075) (layer "F.Fab") (width 0.1) (tstamp 46189e15-73a7-47af-aa31-8f9fe5430069))
    (fp_line (start 7.7 6.67) (end 7.7 -6.71) (layer "F.Fab") (width 0.1) (tstamp 4621e400-0302-4866-ab44-79c576e3c01d))
    (fp_line (start -7.7 6.67) (end 7.7 6.67) (layer "F.Fab") (width 0.1) (tstamp 47b1e64c-e36b-4dc1-a8c3-025e20e305d9))
    (fp_line (start -10.48 1.515) (end -7.7 1.515) (layer "F.Fab") (width 0.1) (tstamp 4a159038-e1a1-404a-bfea-34ead2f311bc))
    (fp_line (start 7.7 -6.078) (end 10.48 -6.078) (layer "F.Fab") (width 0.1) (tstamp 4b0d2ff9-c164-49d4-971c-1ea9c62f013e))
    (fp_line (start 7.7 -4.938) (end 10.48 -4.938) (layer "F.Fab") (width 0.1) (tstamp 4d82cbfd-8f3f-41ff-8ec1-67f0a6bb8e31))
    (fp_line (start -10.48 -0.765) (end -7.7 -0.765) (layer "F.Fab") (width 0.1) (tstamp 5430be09-2dd5-4347-b80c-9e8a120172e8))
    (fp_line (start 7.7 0.765) (end 10.48 0.765) (layer "F.Fab") (width 0.1) (tstamp 5d1c0efb-b256-4edd-b6c6-e342481f1f75))
    (fp_line (start -10.48 3.816) (end -7.7 3.816) (layer "F.Fab") (width 0.1) (tstamp 5f13b95f-acb5-4102-8b38-757d3ba9db3f))
    (fp_line (start -10.48 0.765) (end -10.48 1.515) (layer "F.Fab") (width 0.1) (tstamp 60ab11df-7ec6-4862-a63f-21a5fb7314af))
    (fp_line (start -10.48 1.905) (end -10.48 2.655) (layer "F.Fab") (width 0.1) (tstamp 647c6174-7deb-4ad8-96e7-deb972c4e5c3))
    (fp_line (start -7.7 -4.935) (end -10.48 -4.935) (layer "F.Fab") (width 0.1) (tstamp 6804081d-8b45-458d-9a19-23898a270380))
    (fp_line (start -6.7 -6.71) (end 7.7 -6.71) (layer "F.Fab") (width 0.1) (tstamp 68ae6a90-da1d-4a78-b312-7227cb5695d9))
    (fp_line (start 10.48 4.206) (end 7.7 4.206) (layer "F.Fab") (width 0.1) (tstamp 6a81b739-960e-4ae8-bfd1-6cb2b5d54abd))
    (fp_line (start -10.48 -3.048) (end -7.7 -3.048) (layer "F.Fab") (width 0.1) (tstamp 6bde17d2-ae0b-447f-97ef-42a4f2718343))
    (fp_line (start 10.48 5.334) (end 7.7 5.334) (layer "F.Fab") (width 0.1) (tstamp 6edfdd92-e208-4865-8863-1719479af0b6))
    (fp_line (start -7.7 0.765) (end -10.48 0.765) (layer "F.Fab") (width 0.1) (tstamp 7611f220-c254-4124-967e-a76ea961b438))
    (fp_line (start -7.7 4.206) (end -10.48 4.206) (layer "F.Fab") (width 0.1) (tstamp 7db374c4-c12e-40fb-af8b-10d096e0f3e5))
    (fp_line (start -10.48 -0.375) (end -10.48 0.375) (layer "F.Fab") (width 0.1) (tstamp 7e76fff3-4a16-4554-9e73-73745d73fc9a))
    (fp_line (start -10.48 0.375) (end -7.7 0.375) (layer "F.Fab") (width 0.1) (tstamp 90d375ea-7f4d-4536-858b-4b9304172f6b))
    (fp_line (start 7.7 -3.798) (end 10.48 -3.798) (layer "F.Fab") (width 0.1) (tstamp 910b876e-ca89-4c16-ac14-53a6bc707f92))
    (fp_line (start -10.48 4.956) (end -7.7 4.956) (layer "F.Fab") (width 0.1) (tstamp 96591fd4-f103-454e-a0d9-5dd36648d224))
    (fp_line (start 7.7 -1.515) (end 10.48 -1.515) (layer "F.Fab") (width 0.1) (tstamp 98f19deb-c1d4-4e23-9fcb-5c4c17204212))
    (fp_line (start 10.48 -0.375) (end 10.48 0.375) (layer "F.Fab") (width 0.1) (tstamp 9c2f5325-4248-4072-bef6-585b8e793ab8))
    (fp_line (start 7.7 -2.655) (end 10.48 -2.655) (layer "F.Fab") (width 0.1) (tstamp a12fcd92-fa97-4557-9816-61027d9f3a67))
    (fp_line (start -7.7 3.066) (end -10.48 3.066) (layer "F.Fab") (width 0.1) (tstamp a1cd6989-de33-4825-bdea-941a9cb37c5a))
    (fp_line (start 7.7 1.905) (end 10.48 1.905) (layer "F.Fab") (width 0.1) (tstamp a374c127-7834-4c45-9ff7-87eac19d2c7b))
    (fp_line (start 10.48 3.066) (end 7.7 3.066) (layer "F.Fab") (width 0.1) (tstamp a85aae93-bf7f-4f5b-9698-8eadf0f73625))
    (fp_line (start 10.48 0.375) (end 7.7 0.375) (layer "F.Fab") (width 0.1) (tstamp a8c4cc10-c733-4c4d-841f-01c8a6a861e8))
    (fp_line (start -10.48 -3.795) (end -7.7 -3.795) (layer "F.Fab") (width 0.1) (tstamp b2c4d191-d34b-483e-aa6a-a1feafaa3974))
    (fp_line (start 10.48 -0.765) (end 7.7 -0.765) (layer "F.Fab") (width 0.1) (tstamp b39f992e-f7a9-41de-b021-38c622c21d74))
    (fp_line (start -10.48 6.096) (end -7.7 6.096) (layer "F.Fab") (width 0.1) (tstamp b4b060f7-2b3e-4bed-999d-f50d14e3554a))
    (fp_line (start 10.48 0.765) (end 10.48 1.515) (layer "F.Fab") (width 0.1) (tstamp b6dd281d-709d-40d0-b07a-d66cc5ab1c21))
    (fp_line (start 10.48 -1.905) (end 7.7 -1.905) (layer "F.Fab") (width 0.1) (tstamp b7713136-3236-4d6e-b1c3-0ee4d716ab00))
    (fp_line (start -7.7 -0.375) (end -10.48 -0.375) (layer "F.Fab") (width 0.1) (tstamp c3859b88-ee1c-4daa-9fe4-63386a16086c))
    (fp_line (start -10.48 -5.334) (end -7.7 -5.334) (layer "F.Fab") (width 0.1) (tstamp c4efb39c-5651-4414-86e8-e7a2ce1a9193))
    (fp_line (start 10.48 -2.655) (end 10.48 -1.905) (layer "F.Fab") (width 0.1) (tstamp c56e9b46-40e6-4c99-8309-2c798e0730d0))
    (fp_line (start -7.7 -2.655) (end -10.48 -2.655) (layer "F.Fab") (width 0.1) (tstamp cc20eb37-bbe2-4fec-8de0-7bf8c5192cfc))
    (fp_line (start 10.48 2.655) (end 7.7 2.655) (layer "F.Fab") (width 0.1) (tstamp cd0dd716-3c84-4981-941e-545033f1c88f))
    (fp_line (start -10.48 -1.515) (end -10.48 -0.765) (layer "F.Fab") (width 0.1) (tstamp cd1bac89-4bda-4b0d-b874-c1bd0e41d29c))
    (fp_line (start -7.7 6.67) (end -7.7 -5.71) (layer "F.Fab") (width 0.1) (tstamp da3e30e6-c753-445d-a301-5940cefab900))
    (fp_line (start 7.7 3.816) (end 10.48 3.816) (layer "F.Fab") (width 0.1) (tstamp dabd0e43-eac5-4e80-8b46-939e70028150))
    (fp_line (start -7.7 -4.188) (end -10.48 -4.188) (layer "F.Fab") (width 0.1) (tstamp e0da8c34-c5fa-4114-8401-f99501c7d8fe))
    (fp_line (start 10.534 -4.188) (end 7.754 -4.188) (layer "F.Fab") (width 0.1) (tstamp f0fa9160-66c1-43bd-9112-47c811ec6038))
    (fp_line (start -10.48 -2.655) (end -10.48 -1.905) (layer "F.Fab") (width 0.1) (tstamp f49b200c-1fa1-471e-b489-fb83c7bd21ad))
    (fp_line (start 10.48 -1.515) (end 10.48 -0.765) (layer "F.Fab") (width 0.1) (tstamp fa4643d2-2d29-4206-89d3-2ea6041fc5c2))
    (fp_line (start 7.7 4.956) (end 10.48 4.956) (layer "F.Fab") (width 0.1) (tstamp fe762642-26af-41fe-b977-da3a7107c2e0))
    (pad "1" smd roundrect (at -9.85 -5.7) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "unconnected-(Q1-Pad1)") (pinfunction "Gate") (pintype "input") (tstamp 113db992-658b-4f23-8b16-4522e5d594a2))
    (pad "2" smd roundrect (at -9.85 -4.56) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "unconnected-(Q1-Pad2)") (pinfunction "Driver_Source") (pintype "input") (tstamp 320b70ed-1fda-4e4d-850f-cf0127518540))
    (pad "3" smd roundrect (at -9.85 -3.46) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad10)") (pinfunction "Power_Source") (pintype "passive") (tstamp a0c64033-eec7-4cb3-932e-7f2c7690d9e9))
    (pad "4" smd roundrect (at -9.85 -2.28) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad10)") (pinfunction "Power_Source") (pintype "passive") (tstamp acca42f9-0066-457a-9e94-619dc68348e7))
    (pad "5" smd roundrect (at -9.85 -1.14) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad10)") (pinfunction "Power_Source") (pintype "passive") (tstamp a7f33b7c-283c-4890-90eb-f68bb9988735))
    (pad "6" smd roundrect (at -9.85 0) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad10)") (pinfunction "Power_Source") (pintype "passive") (tstamp 6b3bafb2-a0af-4167-a54b-c7209cf35456))
    (pad "7" smd roundrect (at -9.85 1.14) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad10)") (pinfunction "Power_Source") (pintype "passive") (tstamp dde2e95b-0227-4fbf-9728-da48338bde28))
    (pad "8" smd roundrect (at -9.85 2.28) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad10)") (pinfunction "Power_Source") (pintype "passive") (tstamp 223aede2-dfc2-4a6f-b0b7-5729f94aa508))
    (pad "9" smd roundrect (at -9.85 3.46) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad10)") (pinfunction "Power_Source") (pintype "passive") (tstamp 581d3769-fe5a-4e30-86d6-8cb31fdf34b3))
    (pad "10" smd roundrect (at -9.85 4.56) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad10)") (pinfunction "Power_Source") (pintype "passive") (tstamp 6a9e1a64-3582-4486-9fa6-38d59f40ce68))
    (pad "11" smd roundrect (at -9.85 5.7) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad10)") (pinfunction "Power_Source") (pintype "passive") (tstamp 0711c6db-703f-460a-9dd0-9bb282688338))
    (pad "12" smd roundrect (at 9.652 5.712) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp a4525e50-456e-4d57-9ad8-84d9d1c29cd7))
    (pad "13" smd roundrect (at 9.652 4.572) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp 5c7338df-7f2c-4644-bcf7-f93f1c5a890c))
    (pad "14" smd roundrect (at 9.652 3.472) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp ce1b99f0-cfeb-44a9-b416-0405c9b1d782))
    (pad "15" smd roundrect (at 9.652 2.292) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp afd13723-f725-4478-a0dd-302a63ba6eca))
    (pad "16" smd roundrect (at 9.652 1.152) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp 87848700-7291-40c9-9208-3b80b28f086c))
    (pad "17" smd roundrect (at 9.652 0.012) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp 0f67c8df-54bb-445b-a1dc-00496152a43b))
    (pad "18" smd roundrect (at 9.652 -1.128) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp 91f3de45-8c24-45f3-97b4-fe7909b94d61))
    (pad "19" smd roundrect (at 9.652 -2.268) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp 70b7e318-9519-4c2a-b75d-bcaebf4c3cd1))
    (pad "20" smd roundrect (at 9.652 -3.448) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp a9760ae2-f443-444b-ae2c-b9eb5812916c))
    (pad "21" smd roundrect (at 9.652 -4.548) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+") (pinfunction "Drain") (pintype "passive") (tstamp 7a69a0f6-665c-4adf-b15c-27dd371a4ccd))
    (pad "22" smd roundrect (at 9.652 -5.688) (size 2.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 76bcb8e5-bb31-4036-bc53-507d07eb7e5e))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/Infineon_PG-HDSOP-10-1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
