(footprint "1913_reflow" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62657559)
  (attr smd)
  (fp_text reference "REF**" (at 0 -5.08 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9d88ec4c-16ba-42ca-8cb0-a045e547e117)
  )
  (fp_text value "1913_hand_solder" (at 0 7.62 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a53fdea7-3617-4e29-ba39-1fc4cced14bc)
  )
  (fp_text user "${REFERENCE}" (at 0 10.16 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp df6a19e9-6359-4874-b780-a07aa80e9e7b)
  )
  (fp_line (start -1.6 -1.31) (end 1.6 -1.31) (layer "F.SilkS") (width 0.12) (tstamp 5af55f91-716b-4e7d-8c75-1fd345b7c35e))
  (fp_line (start -1.6 1.31) (end 1.6 1.31) (layer "F.SilkS") (width 0.12) (tstamp b5e82878-b519-4073-ad55-f1d9914c05ff))
  (pad "1" smd roundrect (at 1.35 0) (size 0.9 2.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e2b3c6db-26a0-4a0f-91e3-f3850153add5))
  (pad "2" smd roundrect (at -1.35 0) (size 0.9 2.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ddde8db6-e78c-400a-8a53-c5bb6cc6bdfd))
)
