(footprint "2520" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.3 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 494fbe4d-27ff-4def-98d1-63475a621a20)
  )
  (fp_text value "2520" (at 0 3.65 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 46da2bb5-bcd3-4b08-8f85-4fe3db408e25)
  )
  (fp_text user "${REFERENCE}" (at 0 2.05 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 22935539-075b-4879-abf1-112022464ca7)
  )
  (fp_line (start -0.45 -0.95) (end 0.45 -0.95)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 9ce0302c-d319-4736-a696-28d81bf97996))
  (fp_line (start -0.45 0.95) (end 0.45 0.95)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 72536801-6497-44fb-b8a2-9303d3cbe686))
  (pad "1" smd rect (at -1.05 0) (size 0.9 2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 833d6cf8-45f0-4f7e-8bcb-0f8be8906cfa))
  (pad "2" smd rect (at 1.05 0) (size 0.9 2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp fbba4a42-b7f9-4e06-945e-ff705bca77dd))
)
