(module Panasonic_TQ2SA (layer F.Cu) (tedit 5CB35CBE)
  (fp_text reference REF** (at -7 -0.25 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Panasonic_TQ2SA (at 6.25 0 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6 3) (end -6 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 -3) (end 5.5 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.5 -3) (end 5.5 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.5 3) (end -6 3) (layer F.SilkS) (width 0.15))
  (pad 10 smd rect (at -5.25 -4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -2.71 -4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -0.17 -4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.37 -4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 4.91 -4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -5.25 4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.71 4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.17 4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 2.37 4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 4.91 4.78) (size 1 3) (layers F.Cu F.Paste F.Mask))
)
