/*
 * Intel ACPI Component Architecture
 * AML/ASL+ Disassembler version 20220331 (64-bit version)
 * Copyright (c) 2000 - 2022 Intel Corporation
 * 
 * Disassembling to symbolic ASL+ operators
 *
 * Disassembly of ssdt27.dat, Thu Sep  1 23:24:17 2022
 *
 * Original Table Header:
 *     Signature        "SSDT"
 *     Length           0x000000D9 (217)
 *     Revision         0x01
 *     Checksum         0x9E
 *     OEM ID           "LENOVO"
 *     OEM Table ID     "CB-01   "
 *     OEM Revision     0x00000001 (1)
 *     Compiler ID      "ACPI"
 *     Compiler Version 0x00040000 (262144)
 */
DefinitionBlock ("", "SSDT", 1, "LENOVO", "CB-01   ", 0x00000001)
{
    External (_SB_.PCI0.LPC0.EC0_.DIEH, FieldUnitObj)
    External (_SB_.PCI0.LPC0.EC0_.OKEC, IntObj)
    External (_SB_.PCI0.LPC0.EC0_.Z009, MutexObj)
    External (_SB_.PLTF.C000, DeviceObj)
    External (_SB_.PLTF.C001, DeviceObj)
    External (_SB_.PLTF.C002, DeviceObj)
    External (_SB_.PLTF.C003, DeviceObj)
    External (_SB_.PLTF.C004, DeviceObj)
    External (_SB_.PLTF.C005, DeviceObj)
    External (_SB_.PLTF.C006, DeviceObj)
    External (_SB_.PLTF.C007, DeviceObj)
    External (_SB_.PLTF.C008, DeviceObj)
    External (_SB_.PLTF.C009, DeviceObj)
    External (_SB_.PLTF.C00A, DeviceObj)
    External (_SB_.PLTF.C00B, DeviceObj)
    External (_SB_.PLTF.C00C, DeviceObj)
    External (_SB_.PLTF.C00D, DeviceObj)
    External (_SB_.PLTF.C00E, DeviceObj)
    External (_SB_.PLTF.C00F, DeviceObj)
    External (M037, DeviceObj)
    External (M046, IntObj)
    External (M050, DeviceObj)
    External (M051, DeviceObj)
    External (M052, DeviceObj)
    External (M053, DeviceObj)
    External (M054, DeviceObj)
    External (M055, DeviceObj)
    External (M056, DeviceObj)
    External (M057, DeviceObj)
    External (M058, DeviceObj)
    External (M059, DeviceObj)
    External (M062, DeviceObj)
    External (M068, DeviceObj)
    External (M069, DeviceObj)
    External (M070, DeviceObj)
    External (M071, DeviceObj)
    External (M072, DeviceObj)
    External (M074, DeviceObj)
    External (M075, DeviceObj)
    External (M076, DeviceObj)
    External (M077, DeviceObj)
    External (M078, DeviceObj)
    External (M079, DeviceObj)
    External (M080, DeviceObj)
    External (M081, DeviceObj)
    External (M082, FieldUnitObj)
    External (M083, FieldUnitObj)
    External (M084, FieldUnitObj)
    External (M085, FieldUnitObj)
    External (M086, FieldUnitObj)
    External (M087, FieldUnitObj)
    External (M088, FieldUnitObj)
    External (M089, FieldUnitObj)
    External (M090, FieldUnitObj)
    External (M091, FieldUnitObj)
    External (M092, FieldUnitObj)
    External (M093, FieldUnitObj)
    External (M094, FieldUnitObj)
    External (M095, FieldUnitObj)
    External (M096, FieldUnitObj)
    External (M097, FieldUnitObj)
    External (M098, FieldUnitObj)
    External (M099, FieldUnitObj)
    External (M100, FieldUnitObj)
    External (M101, FieldUnitObj)
    External (M102, FieldUnitObj)
    External (M103, FieldUnitObj)
    External (M104, FieldUnitObj)
    External (M105, FieldUnitObj)
    External (M106, FieldUnitObj)
    External (M107, FieldUnitObj)
    External (M108, FieldUnitObj)
    External (M109, FieldUnitObj)
    External (M110, FieldUnitObj)
    External (M115, BuffObj)
    External (M116, BuffFieldObj)
    External (M117, BuffFieldObj)
    External (M118, BuffFieldObj)
    External (M119, BuffFieldObj)
    External (M120, BuffFieldObj)
    External (M122, FieldUnitObj)
    External (M127, DeviceObj)
    External (M128, FieldUnitObj)
    External (M131, FieldUnitObj)
    External (M132, FieldUnitObj)
    External (M133, FieldUnitObj)
    External (M134, FieldUnitObj)
    External (M135, FieldUnitObj)
    External (M136, FieldUnitObj)
    External (M220, FieldUnitObj)
    External (M221, FieldUnitObj)
    External (M226, FieldUnitObj)
    External (M227, DeviceObj)
    External (M229, FieldUnitObj)
    External (M231, FieldUnitObj)
    External (M233, FieldUnitObj)
    External (M235, FieldUnitObj)
    External (M23A, FieldUnitObj)
    External (M251, FieldUnitObj)
    External (M280, FieldUnitObj)
    External (M290, FieldUnitObj)
    External (M310, FieldUnitObj)
    External (M31C, FieldUnitObj)
    External (M320, FieldUnitObj)
    External (M321, FieldUnitObj)
    External (M322, FieldUnitObj)
    External (M323, FieldUnitObj)
    External (M324, FieldUnitObj)
    External (M325, FieldUnitObj)
    External (M326, FieldUnitObj)
    External (M327, FieldUnitObj)
    External (M328, FieldUnitObj)
    External (M329, DeviceObj)
    External (M32A, DeviceObj)
    External (M32B, DeviceObj)
    External (M330, DeviceObj)
    External (M331, FieldUnitObj)
    External (M378, FieldUnitObj)
    External (M379, FieldUnitObj)
    External (M380, FieldUnitObj)
    External (M381, FieldUnitObj)
    External (M382, FieldUnitObj)
    External (M383, FieldUnitObj)
    External (M384, FieldUnitObj)
    External (M385, FieldUnitObj)
    External (M386, FieldUnitObj)
    External (M387, FieldUnitObj)
    External (M388, FieldUnitObj)
    External (M389, FieldUnitObj)
    External (M390, FieldUnitObj)
    External (M391, FieldUnitObj)
    External (M392, FieldUnitObj)
    External (M404, DeviceObj)
    External (M414, FieldUnitObj)
    External (M444, FieldUnitObj)
    External (M449, FieldUnitObj)
    External (M453, FieldUnitObj)
    External (M454, FieldUnitObj)
    External (M455, FieldUnitObj)
    External (M456, FieldUnitObj)
    External (M457, FieldUnitObj)
    External (M4C0, FieldUnitObj)
    External (M4F0, FieldUnitObj)

    Scope (\_SB)
    {
        OperationRegion (TP80, SystemIO, 0x80, 0x04)
        Field (TP80, DWordAcc, NoLock, Preserve)
        {
            PMTP,   32
        }

        Name (DPX4, 0xA9F40000)
        Method (APX4, 0, Serialized)
        {
            PMTP = DPX4 /* \_SB_.DPX4 */
            DPX4 += One
        }

        Method (APX7, 2, Serialized)
        {
            PMTP = (0xA9F70000 | Arg0)
            Sleep (0x01F4)
            PMTP = Arg1
        }

        Method (APX8, 1, Serialized)
        {
            PMTP = (0xA9F80000 | Arg0)
        }

        Method (APXA, 1, Serialized)
        {
            PMTP = (0xA9FA0000 | Arg0)
        }

        Method (APXE, 3, Serialized)
        {
            PMTP = (0xA9FE0000 | Arg0)
            Sleep (0x01F4)
            PMTP = Arg1
            Sleep (0x01F4)
            PMTP = Arg2
        }
    }
}

