(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "BD9F800MUX" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 20.32 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "BD9F800MUX" (at 0 11.43 90)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Sensum:BD9F800MUX" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/switching_regulator/bd9f800mux-e.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Rohm dcdc converter buck" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "4.5V to 28V Input, 8.0A Integrated MOSFET Single Synchronous Buck DC/DC Converter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BD9F800MUX_0_1"
      (rectangle (start -8.89 20.32) (end 8.89 -17.78)
        (stroke (width 0) (type solid))
        (fill (type none))
      )
    )
    (symbol "BD9F800MUX_1_1"
      (pin power_out line (at 11.43 17.78 180) (length 2.54)
        (name "BOOT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 2.54)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 -15.24 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -11.43 -11.43 0) (length 2.54)
        (name "PGD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 11.43 -2.54 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 -2.54 0) (length 2.54)
        (name "FREQ" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 -11.43 180) (length 2.54)
        (name "FB" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -11.43 7.62 0) (length 2.54)
        (name "VREG" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 -15.24 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -11.43 17.78 0) (length 2.54)
        (name "Vin" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 11.43 7.62 180) (length 2.54)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LMR50410DBV" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 6.35 -16.51 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LMR50410DBV" (at -1.27 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (at 2.54 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmr50410.pdf?ts=1599664184653&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FLMR50410%253Fqgpn%253Dlmr50410" (at 2.54 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Buck DCDC Converter Ti" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "SIMPLE SWITCHER® 4-V to 36-V, 1-A Buck Converter in SOT-23-6 package" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LMR50410DBV_0_1"
      (rectangle (start -5.08 7.62) (end 5.08 -17.78)
        (stroke (width 0) (type solid))
        (fill (type none))
      )
    )
    (symbol "LMR50410DBV_1_1"
      (pin output line (at 7.62 5.08 180) (length 2.54)
        (name "CB" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 7.62 -15.24 180) (length 2.54)
        (name "FB" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -15.24 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 5.08 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 -5.08 180) (length 2.54)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
