(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "TB67H400AFNG,EL" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -10.16 17.78 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TB67H400AFNG" (at 0 -1.27 90)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "350_power_driver_motor_dc:HTSSOP48" (at 20.32 48.26 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://toshiba.semicon-storage.com/us/semiconductor/product/motor-driver-ics/brushed-dc-motor-driver-ics/detail.TB67H400AFNG.html" (at 71.12 45.72 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "man" "toshiba" (at -5.08 50.8 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "man_no" "TB67H400AFNG,EL" (at 10.16 50.8 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "disti" "digikey" (at -5.08 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "disti_no" "TB67H400AFNGELTR-ND" (at 12.7 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TB67H400AFNG,EL_0_0"
      (pin input clock (at -12.7 12.7 0) (length 2.54)
        (name "OSCM" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "TBLKAB" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 1.27 180) (length 2.54)
        (name "OUTA+" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 -1.27 180) (length 2.54)
        (name "OUTA-" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 -10.16 180) (length 2.54)
        (name "OUTB-" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 1.27 0) (length 2.54)
        (name "INA1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -1.27 0) (length 2.54)
        (name "INA2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -3.81 0) (length 2.54)
        (name "PWMA" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 2.54)
        (name "PWMB" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 2.54)
        (name "INB1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 2.54)
        (name "INB2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TB67H400AFNG,EL_0_1"
      (rectangle (start 27.94 -15.24) (end 27.94 -15.24)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "TB67H400AFNG,EL_1_0"
      (pin passive line (at 0 -19.05 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -3.81 180) (length 2.54)
        (name "RSA" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -3.81 180) (length 2.54) hide
        (name "RSA" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 1.27 180) (length 2.54) hide
        (name "OUTA+" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -19.05 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 -1.27 180) (length 2.54) hide
        (name "OUTA-" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -19.05 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -19.05 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 -10.16 180) (length 2.54) hide
        (name "OUTB-" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -19.05 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 -7.62 180) (length 2.54)
        (name "OUTB+" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 12.7 -7.62 180) (length 2.54) hide
        (name "OUTB+" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -12.7 180) (length 2.54)
        (name "RSB" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -12.7 180) (length 2.54) hide
        (name "RSB" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 6.35 19.05 270) (length 2.54)
        (name "VM" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 19.05 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -19.05 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "HBMODE" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TB67H400AFNG,EL_1_1"
      (rectangle (start -10.16 16.51) (end 10.16 -16.51)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
)
