(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "PI4IOE5V6416" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PI4IOE5V6416" (at 0 16.51 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm" (at 21.59 52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/PI4IOE5V6416.pdf" (at 30.48 49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "man" "diodes" (at -5.08 54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "man_no" "PI4IOE5V6416LEX" (at 8.89 54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "disti" "digikey" (at -5.08 46.99 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "disti_no" "PI4IOE5V6416LEXDITR-ND" (at 12.7 46.99 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PI4IOE5V6416_1_0"
      (pin output inverted (at -10.16 12.7 0) (length 2.54)
        (name "~{INT}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -10.16 0) (length 2.54)
        (name "P0_6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -12.7 0) (length 2.54)
        (name "P0_7" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 -15.24 0) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -15.24 180) (length 2.54)
        (name "P1_0" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -12.7 180) (length 2.54)
        (name "P1_1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -10.16 180) (length 2.54)
        (name "P1_2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -7.62 180) (length 2.54)
        (name "P1_3" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -5.08 180) (length 2.54)
        (name "P1_4" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -2.54 180) (length 2.54)
        (name "P1_5" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 0 180) (length 2.54)
        (name "P1_6" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 10.16 0) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 2.54 180) (length 2.54)
        (name "P1_7" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 5.08 180) (length 2.54)
        (name "ADDR" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 10.16 7.62 180) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at 10.16 10.16 180) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 12.7 180) (length 2.54)
        (name "VDDP" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at -10.16 7.62 0) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 5.08 0) (length 2.54)
        (name "P0_0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 2.54 0) (length 2.54)
        (name "P0_1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 0 0) (length 2.54)
        (name "P0_2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -2.54 0) (length 2.54)
        (name "P0_3" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -5.08 0) (length 2.54)
        (name "P0_4" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -7.62 0) (length 2.54)
        (name "P0_5" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "PI4IOE5V6416_1_1"
      (text_box ""
        (at -7.62 15.24 0) (size 15.24 -33.02)
        (stroke (width 0) (type default))
        (fill (type color) (color 0 0 0 0))
        (effects (font (size 1.27 1.27)) (justify left top))
      )
    )
  )
)
