(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "OPA594T" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -11.43 15.24 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "OPA549T" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x2.54mm_StaggerOdd_Lead5.84mm_TabDown" (at 3.81 -26.67 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa549.pdf" (at -2.54 -29.21 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "High-Voltage, High-Current Operational Amplifier" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "OPA594T_0_1"
      (polyline
        (pts
          (xy -7.62 12.7)
          (xy -7.62 -12.7)
          (xy 17.78 0)
          (xy -7.62 12.7)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "OPA594T_1_1"
      (pin power_out line (at 21.59 1.27 180) (length 6.4)
        (name "Vo" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 13.97 270) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 13.97 270) (length 5)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 21.59 -1.27 180) (length 6.4)
        (name "Vo" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 6.35 0) (length 2.54)
        (name "-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -6.35 0) (length 2.54)
        (name "+" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -13.97 90) (length 2.54)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 6.35 -13.97 90) (length 8.2)
        (name "Ref" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -13.97 90) (length 5)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -13.97 90) (length 10.2)
        (name "I_LIM" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 7.62 13.97 270) (length 8.8)
        (name "E/S" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
