(footprint "L_Coilcraft_MSS5131-XXX"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.7 -3.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0fec16cf-e79a-4acc-b396-2c34a8cf739f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "L_Coilcraft_MSS5131-XXX"
		(at 0 4 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "370eff1c-f3e6-4ee4-bc00-389de7eb098a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "40a8eee7-a90b-43da-bbc2-570c4e1c464b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2b78cf96-863c-4263-a149-fb3184742ede")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "18e702d6-6326-4c12-9d7b-2990b00f6ab2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.8 -2.8)
		(end -2.8 -0.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "613729cb-cfcd-4873-b188-f5df55c39623")
	)
	(fp_line
		(start -2.8 -2.8)
		(end -0.8 -2.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e9c050da-7939-4144-b22c-e58dc660c213")
	)
	(fp_line
		(start -1 2.8)
		(end 1 2.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "af5bd081-f590-480f-9318-e256bf71f6b3")
	)
	(fp_line
		(start 2.8 1)
		(end 2.8 -1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1954ef9b-2546-4763-990d-e06ba6ff978c")
	)
	(fp_rect
		(start -2.8 -2.8)
		(end 2.8 2.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "b5ce4c02-713c-4707-940f-c90e5643a706")
	)
	(fp_rect
		(start -2.55 -2.55)
		(end 2.55 2.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "d348c944-0914-4f35-8d77-11a7703baad6")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f58bad1f-4da2-4b04-afc4-85b85bcf38c7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd custom
		(at -1.956406 -1.940002)
		(size 0.6215 0.431)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.583594 1.14) (xy -0.583594 -0.6) (xy 4.496406 -0.6) (xy 4.496406 1.14)
					(arc
						(start 3.816682 1.14)
						(mid 1.956406 -0.085)
						(end 0.09613 1.14)
					)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "4d555452-410c-4462-bff9-f56d39b1c1f4")
	)
	(pad "2" smd custom
		(at 1.956406 1.939998 180)
		(size 0.6215 0.431)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.583594 1.14) (xy -0.583594 -0.6) (xy 4.496406 -0.6) (xy 4.496406 1.14)
					(arc
						(start 3.816682 1.14)
						(mid 1.956406 -0.085)
						(end 0.09613 1.14)
					)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "05f7e1d4-8f1c-4996-91ee-c800d16ed1e4")
	)
)
