(footprint "2824"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 5.08 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ec1f605e-2e0f-475d-9dc2-f4165fb0f536")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "2824"
		(at 0 -5.08 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4a12bfed-45b0-498c-af6e-67b0a60e0065")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "06c1764c-9917-477d-8aaf-d8253bc0522e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d4e7fbca-9eca-4cf0-9b07-5bbd13e79aa4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1932f8ad-ffa7-43cd-aba6-cb577650987a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.54 -3.05)
		(end 2.54 -3.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "355beb19-8d45-4b86-9e5c-31cf40cf3723")
	)
	(fp_line
		(start -2.54 3.05)
		(end 2.54 3.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c22fded5-1e13-4f8d-8f85-611121d37d30")
	)
	(fp_rect
		(start -5.75 -3.25)
		(end 5.75 3.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "3caa7bea-012f-4d5d-b34c-fed664112c4f")
	)
	(fp_text user "${REFERENCE}"
		(at -5.08 5.08 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c94867e7-86e9-40ae-8df5-18ebed567ac5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4.1 0)
		(size 2.5 6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "ca61e469-3fc1-4646-abb7-91a4e7141921")
	)
	(pad "2" smd roundrect
		(at 4.1 0)
		(size 2.5 6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "a03d1a13-0c93-4099-a61e-9a88e17fec44")
	)
)
