(footprint "L_Coilcraft_MSS5131-XXX_handsolder"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.8 -4.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0fec16cf-e79a-4acc-b396-2c34a8cf739f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "L_Coilcraft_MSS5131-XXX_handsolder"
		(at 0 5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "370eff1c-f3e6-4ee4-bc00-389de7eb098a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "40a8eee7-a90b-43da-bbc2-570c4e1c464b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2b78cf96-863c-4263-a149-fb3184742ede")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "18e702d6-6326-4c12-9d7b-2990b00f6ab2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.9 -3.8)
		(end -2.9 -1.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8b18b5bf-ee7b-43a1-802f-de137771ce14")
	)
	(fp_line
		(start -2.9 -3.8)
		(end -0.9 -3.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8caf834b-4f19-460f-8171-193d0849ca33")
	)
	(fp_line
		(start -1 3.8)
		(end 1 3.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f07323c8-88de-48bc-b571-c55a860fc82d")
	)
	(fp_line
		(start 2.8 -1)
		(end 2.8 1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c0a88d17-7000-4da5-a838-8068fed92ae4")
	)
	(fp_rect
		(start -2.9 -3.8)
		(end 2.8 3.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "82ed8c10-8a68-44b6-9133-6377469e090a")
	)
	(fp_rect
		(start -2.55 -2.55)
		(end 2.55 2.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "4b25a853-fece-4fe1-9f70-de956f55ecb8")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0.01 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f58bad1f-4da2-4b04-afc4-85b85bcf38c7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd custom
		(at 0 -3)
		(size 4 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_rect
				(start -2 -0.5)
				(end 2 0.5)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -2.54 2.199998) (xy -2.54 0.459998) (xy 2.54 0.459998) (xy 2.54 2.199998)
					(arc
						(start 1.860276 2.199998)
						(mid 0 0.974998)
						(end -1.860276 2.199998)
					)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "4d555452-410c-4462-bff9-f56d39b1c1f4")
	)
	(pad "2" smd custom
		(at 0 2.999996 180)
		(size 4 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -2.54 2.199998) (xy -2.54 0.459998) (xy 2.54 0.459998) (xy 2.54 2.199998)
					(arc
						(start 1.860276 2.199998)
						(mid 0 0.974998)
						(end -1.860276 2.199998)
					)
				)
				(width 0)
				(fill yes)
			)
			(gr_rect
				(start -2 -0.5)
				(end 2 0.5)
				(width 0)
				(fill yes)
			)
		)
		(uuid "45d234ac-bf94-4db4-b155-ff8dc2540a7f")
	)
)
