(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "PQ2614" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "L" (id 0) (at -2.54 0 90)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PQ2614" (id 1) (at -2.54 0 90)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "man" "bourns" (id 4) (at 15.24 10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "man_no" "PQ2614" (id 5) (at 25.4 10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "dist" "dist" (id 6) (at 15.24 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "dist_no" "dits_no" (id 7) (at 25.4 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Ind" "4.7uH" (id 8) (at 2.54 -2.54 90)
      (effects (font (size 0.635 0.635)))
    )
    (property "Cur" "30A" (id 9) (at 2.54 2.54 90)
      (effects (font (size 0.635 0.635)))
    )
    (property "Res" "1.6 mOhm" (id 10) (at 3.81 0 90)
      (effects (font (size 0.635 0.635)))
    )
    (property "ki_keywords" "inductor choke coil reactor magnetic" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Inductor" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PQ2614_0_1"
      (arc (start 0 -2.54) (mid 0.635 -1.905) (end 0 -1.27)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 0 -1.27) (mid 0.635 -0.635) (end 0 0)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 -3.175)
          (xy -1.27 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 -1.905)
          (xy -1.27 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 -0.635)
          (xy -1.27 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 0.635)
          (xy -1.27 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 1.905)
          (xy -1.27 1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 3.175)
          (xy -1.27 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 -3.81)
          (xy -0.635 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 -3.175)
          (xy -0.635 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 -1.905)
          (xy -0.635 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 -0.635)
          (xy -0.635 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 0.635)
          (xy -0.635 0)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 1.905)
          (xy -0.635 1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.635 3.175)
          (xy -0.635 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 0 0) (mid 0.635 0.635) (end 0 1.27)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start 0 1.27) (mid 0.635 1.905) (end 0 2.54)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "PQ2614_1_1"
      (pin free line (at -7.62 0 0) (length 2.54) hide
        (name "Mnt" (effects (font (size 1.27 1.27))))
        (number "-" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 3.81 270) (length 1.27)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -3.81 90) (length 1.27)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
