(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "VNQ5160K" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -13.97 20.32 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "VNQ5160K-E" (at 0 0 90)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "190_active_high_side_switches:VNQ5160K-E" (at 21.59 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.st.com/content/ccc/resource/technical/document/datasheet/ff/f9/e1/e4/0c/31/41/16/CD00154711.pdf/files/CD00154711.pdf/jcr:content/translations/en.CD00154711.pdf" (at 92.71 39.37 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "man" "stm" (at 2.54 44.45 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "man_no" "VNQ5160K-E" (at 11.43 44.45 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "disti" "digikey" (at 3.81 36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "disti_no" "497-19759-ND" (at 15.24 36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "VNQ5160K_0_1"
      (rectangle (start -13.97 17.78) (end 13.97 -20.32)
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "VNQ5160K_1_1"
      (pin power_in line (at -2.54 20.32 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -16.51 -11.43 0) (length 2.54)
        (name "STATUS4" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -17.78 0) (length 2.54)
        (name "STAT_DIS" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 -16.51 180) (length 2.54)
        (name "OUTPUT4" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 -13.97 180) (length 2.54)
        (name "OUTPUT4" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 -11.43 180) (length 2.54)
        (name "OUTPUT4" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 -7.62 180) (length 2.54)
        (name "OUTPUT3" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 -5.08 180) (length 2.54)
        (name "OUTPUT3" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 -2.54 180) (length 2.54)
        (name "OUTPUT3" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 1.27 180) (length 2.54)
        (name "OUTPUT2" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 3.81 180) (length 2.54)
        (name "OUTPUT2" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 6.35 180) (length 2.54)
        (name "OUTPUT2" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 10.16 180) (length 2.54)
        (name "OUTPUT1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 12.7 180) (length 2.54)
        (name "OUTPUT1" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 15.24 180) (length 2.54)
        (name "OUTPUT1" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 10.16 0) (length 2.54)
        (name "INPUT1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -16.51 7.62 0) (length 2.54)
        (name "STATUS1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 3.81 0) (length 2.54)
        (name "INPUT2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -16.51 1.27 0) (length 2.54)
        (name "STATUS2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -2.54 0) (length 2.54)
        (name "INPUT3" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -16.51 -5.08 0) (length 2.54)
        (name "STATUS3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -8.89 0) (length 2.54)
        (name "INPUT4" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 20.32 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "EPAD" (effects (font (size 0.7 0.7))))
      )
    )
  )
)
