(footprint "cui_rcj_011_RCA" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 626EB1A2)
  (attr smd)
  (fp_text reference "REF**" (at 0 5.08 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 067f156e-d8c3-42da-b1fa-8b1e39934d2d)
  )
  (fp_text value "cui_rcj_011_RCA" (at 0 2.54 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp edf3b9b1-0705-4336-98e1-a00e0437c04e)
  )
  (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1d9aad15-9e62-46f3-b51a-b03ddb985b8d)
  )
  (fp_line (start 4.15 -5.2) (end 5 -5.2) (layer "F.SilkS") (width 0.12) (tstamp 233d9294-e2a8-4276-a643-1b935640b0b8))
  (fp_line (start -4.15 -13.25) (end 0 -13.25) (layer "F.SilkS") (width 0.12) (tstamp 25a37a00-4708-418c-b159-89add89b3c03))
  (fp_line (start 5 -4.5) (end 5 -5.2) (layer "F.SilkS") (width 0.12) (tstamp 8a97a49f-0ee9-48db-9531-6a6b4a0de3b0))
  (fp_line (start 0 -13.25) (end 4.15 -13.25) (layer "F.SilkS") (width 0.12) (tstamp aac414c8-37c2-49bb-98da-3a2bf7a0c553))
  (fp_line (start -5 -5.2) (end -4.15 -5.2) (layer "F.SilkS") (width 0.12) (tstamp b38625bf-f726-4eae-b554-fcff0a7f8573))
  (fp_line (start -5 -4.5) (end -5 -5.2) (layer "F.SilkS") (width 0.12) (tstamp b53b6e09-39d8-40c2-b219-667d536deb36))
  (fp_line (start -4.15 -13.25) (end -4.15 -5.2) (layer "F.SilkS") (width 0.12) (tstamp d56888db-a51e-4614-bad0-dd24a6674238))
  (fp_line (start 4.15 -13.25) (end 4.15 -5.2) (layer "F.SilkS") (width 0.12) (tstamp e1f4f38b-347f-4fc8-93a8-0b1b1641ba44))
  (pad "1" thru_hole circle (at 0 0) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask) (tstamp 356c9688-7afb-43c7-84ee-c68da5d252c7))
  (pad "2" thru_hole circle (at -5 0) (size 3.75 3.75) (drill 2.6) (layers *.Cu *.Mask) (tstamp a32781cb-3bfa-41f4-be57-cc3a82553c23))
  (pad "2" thru_hole circle (at 0 -4.5) (size 3.75 3.75) (drill 2.6) (layers *.Cu *.Mask) (tstamp bd156ba5-7fdc-425a-bb4e-12cab9a343f1))
  (pad "2" thru_hole circle (at 5 0) (size 3.75 3.75) (drill 2.6) (layers *.Cu *.Mask) (tstamp f34b5d89-7cf3-4e4a-9c6c-a455fd1dceeb))
)
