# KED

Kerems and Edwins Develeppoment platform.

08.08.21 Kerem & Edwin

	- Preparing the main implementation (dummy)  of our structure which consists of : 
		- CSL : Chip Support Layer
			- CSL for Raspberry 
			- CSL for STM Nucleo
		- BSL : Board Support Layer 
			- BSL for Raspberry 
			- BSL for Oven Control
		- Project Level
			- Integrate BSL dummy fct. to our main.cpp


INTERFACES 

	- pin
		- pin.h Updated with a header infromation "header" and missing function have benn added. 
		- pin.h Is tagged wiht version 1.0 and will be concidered as the first stalbe implementation
		- pin.h will also be used by other interfaces when they need to initiate alternate functions
 	- USART
		- we need to check what are the standart USART funtinalities and implement them all.
		- usart.h the first implmentation will be made to make sure thte we have a working basis.


PROGRAMMING 
	
	- CPP
		- CPP Classes are taking extreme ammount of code ! 5kB for one class
		- Try to generate a CPP proect with cube to sse if we are missing some flags.  	 


DOCUMENTATION

	- STM-Flash utility 
		- https://www.mankier.com/1/st-flash#Options
		- erasing flash ```st-flash erase```
	- Fun with Linus and why he only wants C 
		- https://www.realworldtech.com/forum/?threadid=104196&curpostid=104299
